Release 8.2.03i - par I.34
Copyright (c) 1995-2006 Xilinx, Inc.  All rights reserved.

Wed Feb 27 14:49:53 2008


INFO: The IO information is provided in three file formats as part of the Place and Route (PAR) process.  These formats are:
1. The <design name>_pad.txt file (this file) designed to provide information on IO usage in a human readable ASCII text format viewable through common text editors.
2. The <design namd>_pad.csv file for use with spreadsheet programs such as MS Excel. This file can also be read by PACE to communicate post PAR IO information.
3. The <design name>.pad file designed for parsing by customers.  It uses the "|" as a data field separator.

INPUT FILE:       labkit_map.ncd
OUTPUT FILE:      labkit_pad.txt
PART TYPE:        xc2v6000
SPEED GRADE:      -4
PACKAGE:          bf957

Pinout by Pin Number:

+----------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------+
|Pin Number|Signal Name         |Pin Usage|Pin Name              |Direction|IO Standard|IO Bank Number|Drive (mA)|Slew Rate|Termination|IOB Delay|Voltage|Constraint|DCI Value|IO Register|Signal Integrity|
+----------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------+
|A2        |                    |         |GND                   |         |           |              |          |         |           |         |       |          |         |           |                |
|A3        |                    |         |GND                   |         |           |              |          |         |           |         |       |          |         |           |                |
|A4        |user3<0>            |IOB      |IO_L21P_1             |INPUT    |LVTTL      |1             |          |         |           |NONE     |       |LOCATED   |         |NO         |NONE            |
|A5        |user3<1>            |IOB      |IO_L21N_1/VREF_1      |INPUT    |LVTTL      |1             |          |         |           |NONE     |       |LOCATED   |         |NO         |NONE            |
|A6        |user3<2>            |IOB      |IO_L22P_1             |INPUT    |LVTTL      |1             |          |         |           |NONE     |       |LOCATED   |         |NO         |NONE            |
|A7        |user3<3>            |IOB      |IO_L22N_1             |INPUT    |LVTTL      |1             |          |         |           |NONE     |       |LOCATED   |         |NO         |NONE            |
|A8        |user1<4>            |IOB      |IO_L29P_1             |INPUT    |LVTTL      |1             |          |         |           |NONE     |       |LOCATED   |         |NO         |NONE            |
|A9        |user1<5>            |IOB      |IO_L29N_1             |INPUT    |LVTTL      |1             |          |         |           |NONE     |       |LOCATED   |         |NO         |NONE            |
|A10       |user1<6>            |IOB      |IO_L53P_1             |INPUT    |LVTTL      |1             |          |         |           |NONE     |       |LOCATED   |         |NO         |NONE            |
|A11       |user1<7>            |IOB      |IO_L53N_1             |INPUT    |LVTTL      |1             |          |         |           |NONE     |       |LOCATED   |         |NO         |NONE            |
|A12       |                    |DIFFM    |IO_L74P_1             |UNUSED   |           |1             |          |         |           |         |       |          |         |           |                |
|A13       |                    |DIFFS    |IO_L74N_1             |UNUSED   |           |1             |          |         |           |         |       |          |         |           |                |
|A14       |user3<22>           |IOB      |IO_L94P_1/VREF_1      |INPUT    |LVTTL      |1             |          |         |           |NONE     |       |LOCATED   |         |NO         |NONE            |
|A15       |user3<23>           |IOB      |IO_L94N_1             |INPUT    |LVTTL      |1             |          |         |           |NONE     |       |LOCATED   |         |NO         |NONE            |
|A16       |                    |         |GND                   |         |           |              |          |         |           |         |       |          |         |           |                |
|A17       |                    |DIFFM    |IO_L96P_0/GCLK4S      |UNUSED   |           |0             |          |         |           |         |       |          |         |           |                |
|A18       |user2<8>            |IOB      |IO_L96N_0/GCLK5P      |INPUT    |LVTTL      |0             |          |         |           |NONE     |       |LOCATED   |         |NO         |NONE            |
|A19       |user2<9>            |IOB      |IO_L76P_0             |INPUT    |LVTTL      |0             |          |         |           |NONE     |       |LOCATED   |         |NO         |NONE            |
|A20       |user2<24>           |IOB      |IO_L76N_0             |INPUT    |LVTTL      |0             |          |         |           |NONE     |       |LOCATED   |         |NO         |NONE            |
|A21       |user2<25>           |IOB      |IO_L70P_0             |INPUT    |LVTTL      |0             |          |         |           |NONE     |       |LOCATED   |         |NO         |NONE            |
|A22       |user2<26>           |IOB      |IO_L70N_0             |INPUT    |LVTTL      |0             |          |         |           |NONE     |       |LOCATED   |         |NO         |NONE            |
|A23       |user2<27>           |IOB      |IO_L52P_0             |INPUT    |LVTTL      |0             |          |         |           |NONE     |       |LOCATED   |         |NO         |NONE            |
|A24       |user2<28>           |IOB      |IO_L52N_0             |INPUT    |LVTTL      |0             |          |         |           |NONE     |       |LOCATED   |         |NO         |NONE            |
|A25       |user4<28>           |IOB      |IO_L27P_0/VREF_0      |INPUT    |LVTTL      |0             |          |         |           |NONE     |       |LOCATED   |         |NO         |NONE            |
|A26       |user4<29>           |IOB      |IO_L27N_0             |INPUT    |LVTTL      |0             |          |         |           |NONE     |       |LOCATED   |         |NO         |NONE            |
|A27       |user4<30>           |IOB      |IO_L06P_0             |INPUT    |LVTTL      |0             |          |         |           |NONE     |       |LOCATED   |         |NO         |NONE            |
|A28       |user4<31>           |IOB      |IO_L06N_0             |INPUT    |LVTTL      |0             |          |         |           |NONE     |       |LOCATED   |         |NO         |NONE            |
|A29       |                    |         |GND                   |         |           |              |          |         |           |         |       |          |         |           |                |
|A30       |                    |         |GND                   |         |           |              |          |         |           |         |       |          |         |           |                |
|AA1       |ram1_data<10>       |IOB      |IO_L68N_3             |INPUT    |LVDCI_33   |3             |          |         |           |NONE     |       |LOCATED   |         |NO         |NONE            |
|AA2       |ram1_data<11>       |IOB      |IO_L53N_3             |INPUT    |LVDCI_33   |3             |          |         |           |NONE     |       |LOCATED   |         |NO         |NONE            |
|AA3       |ram1_data<4>        |IOB      |IO_L50N_3             |INPUT    |LVDCI_33   |3             |          |         |           |NONE     |       |LOCATED   |         |NO         |NONE            |
|AA4       |ram1_data<3>        |IOB      |IO_L52N_3             |INPUT    |LVDCI_33   |3             |          |         |           |NONE     |       |LOCATED   |         |NO         |NONE            |
|AA5       |ram1_data<5>        |IOB      |IO_L72P_3             |INPUT    |LVDCI_33   |3             |          |         |           |NONE     |       |LOCATED   |         |NO         |NONE            |
|AA6       |ram1_we_b           |IOB      |IO_L54N_3             |OUTPUT   |LVDCI_33   |3             |          |NONE*    |NONE**     |         |       |LOCATED   |         |NO         |DRIVER          |
|AA7       |ram1_address<12>    |IOB      |IO_L67P_3             |OUTPUT   |LVDCI_33   |3             |          |NONE*    |NONE**     |         |       |LOCATED   |         |NO         |DRIVER          |
|AA8       |ram1_address<3>     |IOB      |IO_L45P_3             |OUTPUT   |LVDCI_33   |3             |          |NONE*    |NONE**     |         |       |LOCATED   |         |NO         |DRIVER          |
|AA9       |ram1_data<35>       |IOB      |IO_L23N_3             |INPUT    |LVDCI_33   |3             |          |         |           |NONE     |       |LOCATED   |         |NO         |NONE            |
|AA10      |                    |DIFFM    |IO_L27P_3             |UNUSED   |           |3             |          |         |           |         |       |          |         |           |                |
|AA11      |                    |         |VCCINT                |         |           |              |          |         |           |         |1.5    |          |         |           |                |
|AA12      |                    |         |VCCO_4                |         |           |4             |          |         |           |         |3.30   |          |         |           |                |
|AA13      |                    |         |VCCO_4                |         |           |4             |          |         |           |         |3.30   |          |         |           |                |
|AA14      |                    |         |VCCO_4                |         |           |4             |          |         |           |         |3.30   |          |         |           |                |
|AA15      |                    |         |VCCO_4                |         |           |4             |          |         |           |         |3.30   |          |         |           |                |
|AA16      |                    |         |VCCINT                |         |           |              |          |         |           |         |1.5    |          |         |           |                |
|AA17      |                    |         |VCCO_5                |         |           |5             |          |         |           |         |3.30   |          |         |           |                |
|AA18      |                    |         |VCCO_5                |         |           |5             |          |         |           |         |3.30   |          |         |           |                |
|AA19      |                    |         |VCCO_5                |         |           |5             |          |         |           |         |3.30   |          |         |           |                |
|AA20      |                    |         |VCCO_5                |         |           |5             |          |         |           |         |3.30   |          |         |           |                |
|AA21      |                    |         |VCCINT                |         |           |              |          |         |           |         |1.5    |          |         |           |                |
|AA22      |                    |DIFFM    |IO_L19P_6             |UNUSED   |           |6             |          |         |           |         |       |          |         |           |                |
|AA23      |                    |DIFFM    |IO_L44P_6             |UNUSED   |           |6             |          |         |           |         |       |          |         |           |                |
|AA24      |ram0_address<2>     |IOB      |IO_L25N_6             |OUTPUT   |LVDCI_33   |6             |          |NONE*    |NONE**     |         |       |LOCATED   |         |NO         |DRIVER          |
|AA25      |ram0_data<26>       |IOB      |IO_L48P_6             |INPUT    |LVDCI_33   |6             |          |         |           |NONE     |       |LOCATED   |         |NO         |NONE            |
|AA26      |ram0_address<3>     |IOB      |IO_L51P_6             |OUTPUT   |LVDCI_33   |6             |          |NONE*    |NONE**     |         |       |LOCATED   |         |NO         |DRIVER          |
|AA27      |ram0_data<8>        |IOB      |IO_L50N_6             |INPUT    |LVDCI_33   |6             |          |         |           |NONE     |       |LOCATED   |         |NO         |NONE            |
|AA28      |ram0_data<16>       |IOB      |IO_L46N_6             |INPUT    |LVDCI_33   |6             |          |         |           |NONE     |       |LOCATED   |         |NO         |NONE            |
|AA29      |                    |DIFFM    |IO_L70P_6             |UNUSED   |           |6             |          |         |           |         |       |          |         |           |                |
|AA30      |ram0_data<2>        |IOB      |IO_L67N_6             |INPUT    |LVDCI_33   |6             |          |         |           |NONE     |       |LOCATED   |         |NO         |NONE            |
|AA31      |ram0_data<1>        |IOB      |IO_L69N_6/VREF_6      |INPUT    |LVDCI_33   |6             |          |         |           |NONE     |       |LOCATED   |         |NO         |NONE            |
|AB1       |ram1_data<12>       |IOB      |IO_L68P_3             |INPUT    |LVDCI_33   |3             |          |         |           |NONE     |       |LOCATED   |         |NO         |NONE            |
|AB2       |ram1_data<13>       |IOB      |IO_L53P_3             |INPUT    |LVDCI_33   |3             |          |         |           |NONE     |       |LOCATED   |         |NO         |NONE            |
|AB3       |ram1_address<18>    |IOB      |IO_L50P_3             |OUTPUT   |LVDCI_33   |3             |          |NONE*    |NONE**     |         |       |LOCATED   |         |NO         |DRIVER          |
|AB4       |                    |         |GND                   |         |           |              |          |         |           |         |       |          |         |           |                |
|AB5       |                    |DIFFS    |IO_L49N_3             |UNUSED   |           |3             |          |         |           |         |       |          |         |           |                |
|AB6       |                    |         |VCCO_3                |         |           |3             |          |         |           |         |3.30   |          |         |           |                |
|AB7       |ram1_address<11>    |IOB      |IO_L43N_3             |OUTPUT   |LVDCI_33   |3             |          |NONE*    |NONE**     |         |       |LOCATED   |         |NO         |DRIVER          |
|AB8       |ram1_address<4>     |IOB      |IO_L20N_3             |OUTPUT   |LVDCI_33   |3             |          |NONE*    |NONE**     |         |       |LOCATED   |         |NO         |DRIVER          |
|AB9       |ram1_data<26>       |IOB      |IO_L23P_3             |INPUT    |LVDCI_33   |3             |          |         |           |NONE     |       |LOCATED   |         |NO         |NONE            |
|AB10      |                    |DIFFS    |IO_L05N_3             |UNUSED   |           |3             |          |         |           |         |       |          |         |           |                |
|AB11      |                    |DIFFM    |IO_L05P_3             |UNUSED   |           |3             |          |         |           |         |       |          |         |           |                |
|AB12      |button3             |IOB      |IO_L22N_4             |INPUT    |LVTTL      |4             |          |         |           |NONE     |       |LOCATED   |         |NO         |NONE            |
|AB13      |                    |DIFFM    |IO_L22P_4             |UNUSED   |           |4             |          |         |           |         |       |          |         |           |                |
|AB14      |                    |DIFFS    |IO_L76N_4             |UNUSED   |           |4             |          |         |           |         |       |          |         |           |                |
|AB15      |                    |         |VCCINT                |         |           |              |          |         |           |         |1.5    |          |         |           |                |
|AB16      |                    |         |GND                   |         |           |              |          |         |           |         |       |          |         |           |                |
|AB17      |                    |         |VCCINT                |         |           |              |          |         |           |         |1.5    |          |         |           |                |
|AB18      |                    |DIFFM    |IO_L77P_5             |UNUSED   |           |5             |          |         |           |         |       |          |         |           |                |
|AB19      |                    |DIFFS    |IO_L53N_5             |UNUSED   |           |5             |          |         |           |         |       |          |         |           |                |
|AB20      |switch<4>           |IOB      |IO_L53P_5             |INPUT    |LVTTL      |5             |          |         |           |NONE     |       |LOCATED   |         |NO         |NONE            |
|AB21      |tv_in_clock         |IOB      |IO_L20N_5             |OUTPUT   |LVDCI_33   |5             |          |NONE*    |NONE**     |         |       |LOCATED   |         |NO         |DRIVER          |
|AB22      |                    |DIFFM    |IO_L04P_6             |UNUSED   |           |6             |          |         |           |         |       |          |         |           |                |
|AB23      |                    |DIFFS    |IO_L04N_6             |UNUSED   |           |6             |          |         |           |         |       |          |         |           |                |
|AB24      |ram0_address<5>     |IOB      |IO_L25P_6             |OUTPUT   |LVDCI_33   |6             |          |NONE*    |NONE**     |         |       |LOCATED   |         |NO         |DRIVER          |
|AB25      |ram0_data<35>       |IOB      |IO_L27N_6/VREF_6      |INPUT    |LVDCI_33   |6             |          |         |           |NONE     |       |LOCATED   |         |NO         |NONE            |
|AB26      |                    |         |VCCO_6                |         |           |6             |          |         |           |         |3.30   |          |         |           |                |
|AB27      |ram0_address<10>    |IOB      |IO_L50P_6             |OUTPUT   |LVDCI_33   |6             |          |NONE*    |NONE**     |         |       |LOCATED   |         |NO         |DRIVER          |
|AB28      |                    |         |GND                   |         |           |              |          |         |           |         |       |          |         |           |                |
|AB29      |ram0_address<1>     |IOB      |IO_L49N_6             |OUTPUT   |LVDCI_33   |6             |          |NONE*    |NONE**     |         |       |LOCATED   |         |NO         |DRIVER          |
|AB30      |ram0_data<4>        |IOB      |IO_L67P_6             |INPUT    |LVDCI_33   |6             |          |         |           |NONE     |       |LOCATED   |         |NO         |NONE            |
|AB31      |ram0_data<3>        |IOB      |IO_L69P_6             |INPUT    |LVDCI_33   |6             |          |         |           |NONE     |       |LOCATED   |         |NO         |NONE            |
|AC1       |ram1_data<14>       |IOB      |IO_L47N_3             |INPUT    |LVDCI_33   |3             |          |         |           |NONE     |       |LOCATED   |         |NO         |NONE            |
|AC2       |ram1_data<15>       |IOB      |IO_L44N_3             |INPUT    |LVDCI_33   |3             |          |         |           |NONE     |       |LOCATED   |         |NO         |NONE            |
|AC3       |ram1_data<7>        |IOB      |IO_L46N_3             |INPUT    |LVDCI_33   |3             |          |         |           |NONE     |       |LOCATED   |         |NO         |NONE            |
|AC4       |ram1_data<6>        |IOB      |IO_L52P_3             |INPUT    |LVDCI_33   |3             |          |         |           |NONE     |       |LOCATED   |         |NO         |NONE            |
|AC5       |ram1_address<17>    |IOB      |IO_L49P_3             |OUTPUT   |LVDCI_33   |3             |          |NONE*    |NONE**     |         |       |LOCATED   |         |NO         |DRIVER          |
|AC6       |ram1_address<10>    |IOB      |IO_L54P_3             |OUTPUT   |LVDCI_33   |3             |          |NONE*    |NONE**     |         |       |LOCATED   |         |NO         |DRIVER          |
|AC7       |                    |DIFFM    |IO_L43P_3             |UNUSED   |           |3             |          |         |           |         |       |          |         |           |                |
|AC8       |ram1_address<5>     |IOB      |IO_L20P_3             |OUTPUT   |LVDCI_33   |3             |          |NONE*    |NONE**     |         |       |LOCATED   |         |NO         |DRIVER          |
|AC9       |                    |         |GND                   |         |           |              |          |         |           |         |       |          |         |           |                |
|AC10      |vga_out_pixel_clock |IOB      |IO_L19N_4             |OUTPUT   |LVTTL      |4             |12        |SLOW     |NONE**     |         |       |LOCATED   |         |NO         |NONE            |
|AC11      |vga_out_vsync       |IOB      |IO_L19P_4             |OUTPUT   |LVTTL      |4             |12        |SLOW     |NONE**     |         |       |LOCATED   |         |NO         |NONE            |
|AC12      |vga_out_green<0>    |IOB      |IO_L67N_4             |OUTPUT   |LVTTL      |4             |12        |SLOW     |NONE**     |         |       |LOCATED   |         |NO         |NONE            |
|AC13      |vga_out_hsync       |IOB      |IO_L67P_4             |OUTPUT   |LVTTL      |4             |12        |SLOW     |NONE**     |         |       |LOCATED   |         |NO         |NONE            |
|AC14      |vga_out_green<2>    |IOB      |IO_L76P_4             |OUTPUT   |LVTTL      |4             |12        |SLOW     |NONE**     |         |       |LOCATED   |         |NO         |NONE            |
|AC15      |mouse_data          |IOB      |IO_L91N_4/VREF_4      |INPUT    |LVTTL      |4             |          |         |           |NONE     |       |LOCATED   |         |NO         |NONE            |
|AC16      |mouse_clock         |IOB      |IO_L91P_4             |INPUT    |LVTTL      |4             |          |         |           |NONE     |       |LOCATED   |         |NO         |NONE            |
|AC17      |ac97_synch          |IOB      |IO_L77N_5             |OUTPUT   |LVDCI_33   |5             |          |NONE*    |NONE**     |         |       |LOCATED   |         |NO         |DRIVER          |
|AC18      |ac97_sdata_out      |IOB      |IO_L74N_5             |OUTPUT   |LVDCI_33   |5             |          |NONE*    |NONE**     |         |       |LOCATED   |         |NO         |DRIVER          |
|AC19      |beep                |IOB      |IO_L74P_5             |OUTPUT   |LVDCI_33   |5             |          |NONE*    |NONE**     |         |       |LOCATED   |         |NO         |DRIVER          |
|AC20      |switch<5>           |IOB      |IO_L29N_5             |INPUT    |LVTTL      |5             |          |         |           |NONE     |       |LOCATED   |         |NO         |NONE            |
|AC21      |switch<3>           |IOB      |IO_L29P_5             |INPUT    |LVTTL      |5             |          |         |           |IFD      |       |LOCATED   |         |YES        |NONE            |
|AC22      |tv_in_fifo_read     |IOB      |IO_L20P_5             |OUTPUT   |LVDCI_33   |5             |          |NONE*    |NONE**     |         |       |LOCATED   |         |NO         |DRIVER          |
|AC23      |                    |         |GND                   |         |           |              |          |         |           |         |       |          |         |           |                |
|AC24      |ram0_address<14>    |IOB      |IO_L20N_6             |OUTPUT   |LVDCI_33   |6             |          |NONE*    |NONE**     |         |       |LOCATED   |         |NO         |DRIVER          |
|AC25      |ram0_address<4>     |IOB      |IO_L27P_6             |OUTPUT   |LVDCI_33   |6             |          |NONE*    |NONE**     |         |       |LOCATED   |         |NO         |DRIVER          |
|AC26      |ram0_address<0>     |IOB      |IO_L22N_6             |OUTPUT   |LVDCI_33   |6             |          |NONE*    |NONE**     |         |       |LOCATED   |         |NO         |DRIVER          |
|AC27      |ram0_address<11>    |IOB      |IO_L47N_6             |OUTPUT   |LVDCI_33   |6             |          |NONE*    |NONE**     |         |       |LOCATED   |         |NO         |DRIVER          |
|AC28      |                    |DIFFM    |IO_L46P_6             |UNUSED   |           |6             |          |         |           |         |       |          |         |           |                |
|AC29      |                    |DIFFM    |IO_L49P_6             |UNUSED   |           |6             |          |         |           |         |       |          |         |           |                |
|AC30      |ram0_data<6>        |IOB      |IO_L45N_6/VREF_6      |INPUT    |LVDCI_33   |6             |          |         |           |NONE     |       |LOCATED   |         |NO         |NONE            |
|AC31      |ram0_data<5>        |IOB      |IO_L52N_6             |INPUT    |LVDCI_33   |6             |          |         |           |NONE     |       |LOCATED   |         |NO         |NONE            |
|AD1       |ram1_data<16>       |IOB      |IO_L47P_3             |INPUT    |LVDCI_33   |3             |          |         |           |NONE     |       |LOCATED   |         |NO         |NONE            |
|AD2       |                    |         |GND                   |         |           |              |          |         |           |         |       |          |         |           |                |
|AD3       |ram1_address<9>     |IOB      |IO_L46P_3             |OUTPUT   |LVDCI_33   |3             |          |NONE*    |NONE**     |         |       |LOCATED   |         |NO         |DRIVER          |
|AD4       |ram1_address<8>     |IOB      |IO_L22N_3             |OUTPUT   |LVDCI_33   |3             |          |NONE*    |NONE**     |         |       |LOCATED   |         |NO         |DRIVER          |
|AD5       |ram1_data<18>       |IOB      |IO_L21N_3/VREF_3      |INPUT    |LVDCI_33   |3             |          |         |           |NONE     |       |LOCATED   |         |NO         |NONE            |
|AD6       |                    |DIFFS    |IO_L03N_3/VREF_3      |UNUSED   |           |3             |          |         |           |         |       |          |         |           |                |
|AD7       |ram1_address<0>     |IOB      |IO_L03P_3             |OUTPUT   |LVDCI_33   |3             |          |NONE*    |NONE**     |         |       |LOCATED   |         |NO         |DRIVER          |
|AD8       |                    |         |GND                   |         |           |              |          |         |           |         |       |          |         |           |                |
|AD9       |analyzer4_clock     |IOB      |IO_L01N_4/DOUT        |OUTPUT   |LVTTL      |4             |12        |SLOW     |NONE**     |         |       |LOCATED   |         |NO         |NONE            |
|AD10      |                    |DIFFM    |IO_L01P_4/INIT_B      |UNUSED   |           |4             |          |         |           |         |       |          |         |           |                |
|AD11      |button2             |IOB      |IO_L28N_4             |INPUT    |LVTTL      |4             |          |         |           |NONE     |       |LOCATED   |         |NO         |NONE            |
|AD12      |vga_out_red<5>      |IOB      |IO_L28P_4             |OUTPUT   |LVTTL      |4             |12        |SLOW     |NONE**     |         |       |LOCATED   |         |NO         |NONE            |
|AD13      |analyzer4_data<3>   |IOB      |IO_L70N_4             |OUTPUT   |LVTTL      |4             |12        |SLOW     |NONE**     |         |       |LOCATED   |         |NO         |NONE            |
|AD14      |                    |         |VCCO_4                |         |           |4             |          |         |           |         |3.30   |          |         |           |                |
|AD15      |vga_out_green<3>    |IOB      |IO_L70P_4             |OUTPUT   |LVTTL      |4             |12        |SLOW     |NONE**     |         |       |LOCATED   |         |NO         |NONE            |
|AD16      |tv_in_line_clock1   |IOB      |IO_L95N_5/GCLK5S      |INPUT    |LVDCI_33   |5             |          |         |           |NONE     |       |LOCATED   |         |NO         |NONE            |
|AD17      |tv_in_line_clock2   |IOB      |IO_L95P_5/GCLK4P      |INPUT    |LVDCI_33   |5             |          |         |           |NONE     |       |LOCATED   |         |NO         |NONE            |
|AD18      |                    |         |VCCO_5                |         |           |5             |          |         |           |         |3.30   |          |         |           |                |
|AD19      |tv_in_i2c_data      |IOB      |IO_L68N_5             |INPUT    |LVDCI_33   |5             |          |         |           |NONE     |       |LOCATED   |         |NO         |NONE            |
|AD20      |tv_in_ycrcb<13>     |IOB      |IO_L68P_5             |INPUT    |LVTTL      |5             |          |         |           |NONE     |       |LOCATED   |         |NO         |NONE            |
|AD21      |tv_in_i2c_clock     |IOB      |IO_L26N_5             |OUTPUT   |LVDCI_33   |5             |          |NONE*    |NONE**     |         |       |LOCATED   |         |NO         |DRIVER          |
|AD22      |switch<7>           |IOB      |IO_L26P_5             |INPUT    |LVTTL      |5             |          |         |           |NONE     |       |LOCATED   |         |NO         |NONE            |
|AD23      |                    |DIFFS    |IO_L05N_5/VRP_5       |UNUSED   |           |5             |          |         |TERMINATION|         |       |          |         |           |                |
|AD24      |                    |         |GND                   |         |           |              |          |         |           |         |       |          |         |           |                |
|AD25      |ram0_data<27>       |IOB      |IO_L20P_6             |INPUT    |LVDCI_33   |6             |          |         |           |NONE     |       |LOCATED   |         |NO         |NONE            |
|AD26      |ram0_address<13>    |IOB      |IO_L22P_6             |OUTPUT   |LVDCI_33   |6             |          |NONE*    |NONE**     |         |       |LOCATED   |         |NO         |DRIVER          |
|AD27      |ram0_address<12>    |IOB      |IO_L47P_6             |OUTPUT   |LVDCI_33   |6             |          |NONE*    |NONE**     |         |       |LOCATED   |         |NO         |DRIVER          |
|AD28      |ram0_address<16>    |IOB      |IO_L24N_6             |OUTPUT   |LVDCI_33   |6             |          |NONE*    |NONE**     |         |       |LOCATED   |         |NO         |DRIVER          |
|AD29      |ram0_address<15>    |IOB      |IO_L23N_6             |OUTPUT   |LVDCI_33   |6             |          |NONE*    |NONE**     |         |       |LOCATED   |         |NO         |DRIVER          |
|AD30      |                    |         |GND                   |         |           |              |          |         |           |         |       |          |         |           |                |
|AD31      |ram0_data<7>        |IOB      |IO_L52P_6             |INPUT    |LVDCI_33   |6             |          |         |           |NONE     |       |LOCATED   |         |NO         |NONE            |
|AE1       |ram1_data<27>       |IOB      |IO_L25N_3             |INPUT    |LVDCI_33   |3             |          |         |           |NONE     |       |LOCATED   |         |NO         |NONE            |
|AE2       |ram1_data<28>       |IOB      |IO_L44P_3             |INPUT    |LVDCI_33   |3             |          |         |           |NONE     |       |LOCATED   |         |NO         |NONE            |
|AE3       |                    |         |VCCO_3                |         |           |3             |          |         |           |         |3.30   |          |         |           |                |
|AE4       |ram1_data<20>       |IOB      |IO_L22P_3             |INPUT    |LVDCI_33   |3             |          |         |           |NONE     |       |LOCATED   |         |NO         |NONE            |
|AE5       |ram1_data<19>       |IOB      |IO_L21P_3             |INPUT    |LVDCI_33   |3             |          |         |           |NONE     |       |LOCATED   |         |NO         |NONE            |
|AE6       |                    |DIFFS    |IO_L02N_3/VRP_3       |UNUSED   |           |3             |          |         |TERMINATION|         |       |          |         |           |                |
|AE7       |                    |         |GND                   |         |           |              |          |         |           |         |       |          |         |           |                |
|AE8       |vga_out_red<6>      |IOB      |IO_L04N_4/VREF_4      |OUTPUT   |LVTTL      |4             |12        |SLOW     |NONE**     |         |       |LOCATED   |         |NO         |NONE            |
|AE9       |vga_out_red<7>      |IOB      |IO_L20N_4             |OUTPUT   |LVTTL      |4             |12        |SLOW     |NONE**     |         |       |LOCATED   |         |NO         |NONE            |
|AE10      |button1             |IOB      |IO_L20P_4             |INPUT    |LVTTL      |4             |          |         |           |NONE     |       |LOCATED   |         |NO         |NONE            |
|AE11      |button0             |IOB      |IO_L49N_4             |INPUT    |LVTTL      |4             |          |         |           |NONE     |       |LOCATED   |         |NO         |NONE            |
|AE12      |disp_data_in        |IOB      |IO_L49P_4             |INPUT    |LVTTL      |4             |          |         |           |NONE     |       |LOCATED   |         |NO         |NONE            |
|AE13      |                    |         |GND                   |         |           |              |          |         |           |         |       |          |         |           |                |
|AE14      |flash_address<1>    |IOB      |IO_L73N_4             |OUTPUT   |LVTTL      |4             |12        |SLOW     |NONE**     |         |       |LOCATED   |         |NO         |NONE            |
|AE15      |disp_data_out       |IOB      |IO_L73P_4             |OUTPUT   |LVDCI_33   |4             |          |NONE*    |NONE**     |         |       |LOCATED   |         |NO         |DRIVER          |
|AE16      |                    |         |GND                   |         |           |              |          |         |           |         |       |          |         |           |                |
|AE17      |led<7>              |IOB      |IO_L92N_5             |OUTPUT   |LVTTL      |5             |12        |SLOW     |NONE**     |         |       |LOCATED   |         |NO         |NONE            |
|AE18      |audio_reset_b       |IOB      |IO_L92P_5             |OUTPUT   |LVTTL      |5             |12        |SLOW     |NONE**     |         |       |LOCATED   |         |NO         |NONE            |
|AE19      |                    |         |GND                   |         |           |              |          |         |           |         |       |          |         |           |                |
|AE20      |tv_in_ycrcb<15>     |IOB      |IO_L50N_5             |INPUT    |LVTTL      |5             |          |         |           |NONE     |       |LOCATED   |         |NO         |NONE            |
|AE21      |led<1>              |IOB      |IO_L50P_5             |OUTPUT   |LVTTL      |5             |12        |SLOW     |NONE**     |         |       |LOCATED   |         |NO         |NONE            |
|AE22      |led<0>              |IOB      |IO_L23N_5             |OUTPUT   |LVTTL      |5             |12        |SLOW     |NONE**     |         |       |LOCATED   |         |NO         |NONE            |
|AE23      |switch<6>           |IOB      |IO_L23P_5             |INPUT    |LVTTL      |5             |          |         |           |NONE     |       |LOCATED   |         |NO         |NONE            |
|AE24      |                    |DIFFM    |IO_L05P_5/VRN_5       |UNUSED   |           |5             |          |         |TERMINATION|         |       |          |         |           |                |
|AE25      |                    |         |GND                   |         |           |              |          |         |           |         |       |          |         |           |                |
|AE26      |                    |DIFFM    |IO_L02P_6/VRN_6       |UNUSED   |           |6             |          |         |TERMINATION|         |       |          |         |           |                |
|AE27      |                    |DIFFS    |IO_L02N_6/VRP_6       |UNUSED   |           |6             |          |         |TERMINATION|         |       |          |         |           |                |
|AE28      |ram0_data<28>       |IOB      |IO_L24P_6             |INPUT    |LVDCI_33   |6             |          |         |           |NONE     |       |LOCATED   |         |NO         |NONE            |
|AE29      |                    |         |VCCO_6                |         |           |6             |          |         |           |         |3.30   |          |         |           |                |
|AE30      |ram0_data<19>       |IOB      |IO_L45P_6             |INPUT    |LVDCI_33   |6             |          |         |           |NONE     |       |LOCATED   |         |NO         |NONE            |
|AE31      |ram0_data<18>       |IOB      |IO_L43N_6             |INPUT    |LVDCI_33   |6             |          |         |           |NONE     |       |LOCATED   |         |NO         |NONE            |
|AF1       |ram1_data<29>       |IOB      |IO_L25P_3             |INPUT    |LVDCI_33   |3             |          |         |           |NONE     |       |LOCATED   |         |NO         |NONE            |
|AF2       |ram1_data<30>       |IOB      |IO_L24N_3             |INPUT    |LVDCI_33   |3             |          |         |           |NONE     |       |LOCATED   |         |NO         |NONE            |
|AF3       |ram1_data<21>       |IOB      |IO_L04N_3             |INPUT    |LVDCI_33   |3             |          |         |           |NONE     |       |LOCATED   |         |NO         |NONE            |
|AF4       |ram1_data<22>       |IOB      |IO_L06N_3             |INPUT    |LVDCI_33   |3             |          |         |           |NONE     |       |LOCATED   |         |NO         |NONE            |
|AF5       |                    |DIFFM    |IO_L02P_3/VRN_3       |UNUSED   |           |3             |          |         |TERMINATION|         |       |          |         |           |                |
|AF6       |                    |         |GND                   |         |           |              |          |         |           |         |       |          |         |           |                |
|AF7       |                    |DIFFS    |IO_L02N_4/D0          |UNUSED   |           |4             |          |         |           |         |       |          |         |           |                |
|AF8       |vga_out_red<4>      |IOB      |IO_L04P_4             |OUTPUT   |LVTTL      |4             |12        |SLOW     |NONE**     |         |       |LOCATED   |         |NO         |NONE            |
|AF9       |vga_out_red<3>      |IOB      |IO_L26N_4             |OUTPUT   |LVTTL      |4             |12        |SLOW     |NONE**     |         |       |LOCATED   |         |NO         |NONE            |
|AF10      |                    |         |VCCO_4                |         |           |4             |          |         |           |         |3.30   |          |         |           |                |
|AF11      |vga_out_red<0>      |IOB      |IO_L26P_4             |OUTPUT   |LVTTL      |4             |12        |SLOW     |NONE**     |         |       |LOCATED   |         |NO         |NONE            |
|AF12      |disp_blank          |IOB      |IO_L52N_4             |OUTPUT   |LVDCI_33   |4             |          |NONE*    |NONE**     |         |       |LOCATED   |         |NO         |DRIVER          |
|AF13      |disp_ce_b           |IOB      |IO_L52P_4             |OUTPUT   |LVDCI_33   |4             |          |NONE*    |NONE**     |         |       |LOCATED   |         |NO         |DRIVER          |
|AF14      |disp_clock          |IOB      |IO_L74N_4             |OUTPUT   |LVDCI_33   |4             |          |NONE*    |NONE**     |         |       |LOCATED   |         |NO         |DRIVER          |
|AF15      |disp_rs             |IOB      |IO_L74P_4             |OUTPUT   |LVDCI_33   |4             |          |NONE*    |NONE**     |         |       |LOCATED   |         |NO         |DRIVER          |
|AF16      |keyboard_data       |IOB      |IO_L94N_4/VREF_4      |INPUT    |LVTTL      |4             |          |         |           |NONE     |       |LOCATED   |         |NO         |NONE            |
|AF17      |led<6>              |IOB      |IO_L93P_5             |OUTPUT   |LVTTL      |5             |12        |SLOW     |NONE**     |         |       |LOCATED   |         |NO         |NONE            |
|AF18      |led<5>              |IOB      |IO_L71N_5             |OUTPUT   |LVTTL      |5             |12        |SLOW     |NONE**     |         |       |LOCATED   |         |NO         |NONE            |
|AF19      |led<4>              |IOB      |IO_L71P_5             |OUTPUT   |LVTTL      |5             |12        |SLOW     |NONE**     |         |       |LOCATED   |         |NO         |NONE            |
|AF20      |led<3>              |IOB      |IO_L51N_5/VREF_5      |OUTPUT   |LVTTL      |5             |12        |SLOW     |NONE**     |         |       |LOCATED   |         |NO         |NONE            |
|AF21      |tv_in_ycrcb<14>     |IOB      |IO_L51P_5             |INPUT    |LVTTL      |5             |          |         |           |NONE     |       |LOCATED   |         |NO         |NONE            |
|AF22      |                    |         |VCCO_5                |         |           |5             |          |         |           |         |3.30   |          |         |           |                |
|AF23      |analyzer4_data<7>   |IOB      |IO_L03N_5/D4/ALT_VRP_5|OUTPUT   |LVTTL      |5             |12        |SLOW     |NONE**     |         |       |LOCATED   |         |NO         |NONE            |
|AF24      |analyzer4_data<8>   |IOB      |IO_L03P_5/D5/ALT_VRN_5|OUTPUT   |LVTTL      |5             |12        |SLOW     |NONE**     |         |       |LOCATED   |         |NO         |NONE            |
|AF25      |analyzer4_data<10>  |IOB      |IO_L02P_5/D7          |OUTPUT   |LVTTL      |5             |12        |SLOW     |NONE**     |         |       |LOCATED   |         |NO         |NONE            |
|AF26      |                    |         |GND                   |         |           |              |          |         |           |         |       |          |         |           |                |
|AF27      |ram0_data<31>       |IOB      |IO_L01P_6             |INPUT    |LVDCI_33   |6             |          |         |           |NONE     |       |LOCATED   |         |NO         |NONE            |
|AF28      |ram0_data<29>       |IOB      |IO_L01N_6             |INPUT    |LVDCI_33   |6             |          |         |           |NONE     |       |LOCATED   |         |NO         |NONE            |
|AF29      |ram0_data<30>       |IOB      |IO_L23P_6             |INPUT    |LVDCI_33   |6             |          |         |           |NONE     |       |LOCATED   |         |NO         |NONE            |
|AF30      |ram0_data<21>       |IOB      |IO_L21N_6/VREF_6      |INPUT    |LVDCI_33   |6             |          |         |           |NONE     |       |LOCATED   |         |NO         |NONE            |
|AF31      |ram0_data<20>       |IOB      |IO_L43P_6             |INPUT    |LVDCI_33   |6             |          |         |           |NONE     |       |LOCATED   |         |NO         |NONE            |
|AG1       |ram1_data<31>       |IOB      |IO_L19N_3             |INPUT    |LVDCI_33   |3             |          |         |           |NONE     |       |LOCATED   |         |NO         |NONE            |
|AG2       |ram1_data<32>       |IOB      |IO_L24P_3             |INPUT    |LVDCI_33   |3             |          |         |           |NONE     |       |LOCATED   |         |NO         |NONE            |
|AG3       |ram1_data<23>       |IOB      |IO_L04P_3             |INPUT    |LVDCI_33   |3             |          |         |           |NONE     |       |LOCATED   |         |NO         |NONE            |
|AG4       |ram1_data<24>       |IOB      |IO_L06P_3             |INPUT    |LVDCI_33   |3             |          |         |           |NONE     |       |LOCATED   |         |NO         |NONE            |
|AG5       |                    |         |GND                   |         |           |              |          |         |           |         |       |          |         |           |                |
|AG6       |                    |         |DONE                  |         |           |              |          |         |           |         |       |          |         |           |                |
|AG7       |analyzer4_data<15>  |IOB      |IO_L02P_4/D1          |OUTPUT   |LVTTL      |4             |12        |SLOW     |NONE**     |         |       |LOCATED   |         |NO         |NONE            |
|AG8       |vga_out_green<1>    |IOB      |IO_L25N_4             |OUTPUT   |LVTTL      |4             |12        |SLOW     |NONE**     |         |       |LOCATED   |         |NO         |NONE            |
|AG9       |vga_out_red<2>      |IOB      |IO_L25P_4             |OUTPUT   |LVTTL      |4             |12        |SLOW     |NONE**     |         |       |LOCATED   |         |NO         |NONE            |
|AG10      |vga_out_red<1>      |IOB      |IO_L50N_4             |OUTPUT   |LVTTL      |4             |12        |SLOW     |NONE**     |         |       |LOCATED   |         |NO         |NONE            |
|AG11      |disp_reset_b        |IOB      |IO_L50P_4             |OUTPUT   |LVDCI_33   |4             |          |NONE*    |NONE**     |         |       |LOCATED   |         |NO         |DRIVER          |
|AG12      |vga_out_blue<4>     |IOB      |IO_L68N_4             |OUTPUT   |LVTTL      |4             |12        |SLOW     |NONE**     |         |       |LOCATED   |         |NO         |NONE            |
|AG13      |vga_out_blue<5>     |IOB      |IO_L68P_4             |OUTPUT   |LVTTL      |4             |12        |SLOW     |NONE**     |         |       |LOCATED   |         |NO         |NONE            |
|AG14      |vga_out_blue<6>     |IOB      |IO_L92N_4             |OUTPUT   |LVTTL      |4             |12        |SLOW     |NONE**     |         |       |LOCATED   |         |NO         |NONE            |
|AG15      |vga_out_blue<7>     |IOB      |IO_L92P_4             |OUTPUT   |LVTTL      |4             |12        |SLOW     |NONE**     |         |       |LOCATED   |         |NO         |NONE            |
|AG16      |keyboard_clock      |IOB      |IO_L94P_4             |INPUT    |LVTTL      |4             |          |         |           |NONE     |       |LOCATED   |         |NO         |NONE            |
|AG17      |tv_in_ycrcb<19>     |IOB      |IO_L93N_5             |INPUT    |LVTTL      |5             |          |         |           |NONE     |       |LOCATED   |         |NO         |NONE            |
|AG18      |tv_in_ycrcb<18>     |IOB      |IO_L72N_5             |INPUT    |LVTTL      |5             |          |         |           |NONE     |       |LOCATED   |         |NO         |NONE            |
|AG19      |tv_in_ycrcb<17>     |IOB      |IO_L72P_5             |INPUT    |LVTTL      |5             |          |         |           |NONE     |       |LOCATED   |         |NO         |NONE            |
|AG20      |tv_in_ycrcb<16>     |IOB      |IO_L54N_5             |INPUT    |LVTTL      |5             |          |         |           |NONE     |       |LOCATED   |         |NO         |NONE            |
|AG21      |led<2>              |IOB      |IO_L54P_5             |OUTPUT   |LVTTL      |5             |12        |SLOW     |NONE**     |         |       |LOCATED   |         |NO         |NONE            |
|AG22      |tv_in_fifo_clock    |IOB      |IO_L24N_5             |OUTPUT   |LVDCI_33   |5             |          |NONE*    |NONE**     |         |       |LOCATED   |         |NO         |DRIVER          |
|AG23      |tv_in_ycrcb<12>     |IOB      |IO_L24P_5             |INPUT    |LVTTL      |5             |          |         |           |NONE     |       |LOCATED   |         |NO         |NONE            |
|AG24      |analyzer4_data<9>   |IOB      |IO_L02N_5/D6          |OUTPUT   |LVTTL      |5             |12        |SLOW     |NONE**     |         |       |LOCATED   |         |NO         |NONE            |
|AG25      |tv_in_reset_b       |IOB      |IO_L21P_5             |OUTPUT   |LVDCI_33   |5             |          |NONE*    |NONE**     |         |       |LOCATED   |         |NO         |DRIVER          |
|AG26      |                    |         |M2                    |         |           |              |          |         |           |         |       |          |         |           |                |
|AG27      |                    |         |GND                   |         |           |              |          |         |           |         |       |          |         |           |                |
|AG28      |ram0_data<33>       |IOB      |IO_L05P_6             |INPUT    |LVDCI_33   |6             |          |         |           |NONE     |       |LOCATED   |         |NO         |NONE            |
|AG29      |ram0_data<32>       |IOB      |IO_L05N_6             |INPUT    |LVDCI_33   |6             |          |         |           |NONE     |       |LOCATED   |         |NO         |NONE            |
|AG30      |ram0_data<23>       |IOB      |IO_L21P_6             |INPUT    |LVDCI_33   |6             |          |         |           |NONE     |       |LOCATED   |         |NO         |NONE            |
|AG31      |ram0_data<22>       |IOB      |IO_L06N_6             |INPUT    |LVDCI_33   |6             |          |         |           |NONE     |       |LOCATED   |         |NO         |NONE            |
|AH1       |ram1_data<33>       |IOB      |IO_L19P_3             |INPUT    |LVDCI_33   |3             |          |         |           |NONE     |       |LOCATED   |         |NO         |NONE            |
|AH2       |ram1_data<34>       |IOB      |IO_L01N_3             |INPUT    |LVDCI_33   |3             |          |         |           |NONE     |       |LOCATED   |         |NO         |NONE            |
|AH3       |ram1_data<25>       |IOB      |IO_L01P_3             |INPUT    |LVDCI_33   |3             |          |         |           |NONE     |       |LOCATED   |         |NO         |NONE            |
|AH4       |                    |         |GND                   |         |           |              |          |         |           |         |       |          |         |           |                |
|AH5       |                    |         |PWRDWN_B              |         |           |              |          |         |           |         |       |          |         |           |                |
|AH6       |vga_out_green<4>    |IOB      |IO_L06N_4             |OUTPUT   |LVTTL      |4             |12        |SLOW     |NONE**     |         |       |LOCATED   |         |NO         |NONE            |
|AH7       |vga_out_green<6>    |IOB      |IO_L06P_4             |OUTPUT   |LVTTL      |4             |12        |SLOW     |NONE**     |         |       |LOCATED   |         |NO         |NONE            |
|AH8       |vga_out_green<7>    |IOB      |IO_L27N_4             |OUTPUT   |LVTTL      |4             |12        |SLOW     |NONE**     |         |       |LOCATED   |         |NO         |NONE            |
|AH9       |vga_out_blue<0>     |IOB      |IO_L27P_4/VREF_4      |OUTPUT   |LVTTL      |4             |12        |SLOW     |NONE**     |         |       |LOCATED   |         |NO         |NONE            |
|AH10      |                    |         |GND                   |         |           |              |          |         |           |         |       |          |         |           |                |
|AH11      |vga_out_blue<2>     |IOB      |IO_L54N_4             |OUTPUT   |LVTTL      |4             |12        |SLOW     |NONE**     |         |       |LOCATED   |         |NO         |NONE            |
|AH12      |flash_data<9>       |IOB      |IO_L54P_4             |INPUT    |LVTTL      |4             |          |         |           |NONE     |       |LOCATED   |         |NO         |NONE            |
|AH13      |flash_data<8>       |IOB      |IO_L77N_4             |INPUT    |LVTTL      |4             |          |         |           |NONE     |       |LOCATED   |         |NO         |NONE            |
|AH14      |flash_address<0>    |IOB      |IO_L77P_4             |OUTPUT   |LVTTL      |4             |12        |SLOW     |NONE**     |         |       |LOCATED   |         |NO         |NONE            |
|AH15      |flash_byte_b        |IOB      |IO_L96N_4/GCLK1S      |OUTPUT   |LVDCI_33   |4             |          |NONE*    |NONE**     |         |       |LOCATED   |         |NO         |DRIVER          |
|AH16      |                    |         |GND                   |         |           |              |          |         |           |         |       |          |         |           |                |
|AH17      |analyzer4_data<4>   |IOB      |IO_L96P_5/GCLK6P      |OUTPUT   |LVTTL      |5             |12        |SLOW     |NONE**     |         |       |LOCATED   |         |NO         |NONE            |
|AH18      |flash_address<3>    |IOB      |IO_L76N_5             |OUTPUT   |LVTTL      |5             |12        |SLOW     |NONE**     |         |       |LOCATED   |         |NO         |NONE            |
|AH19      |flash_address<4>    |IOB      |IO_L76P_5             |OUTPUT   |LVTTL      |5             |12        |SLOW     |NONE**     |         |       |LOCATED   |         |NO         |NONE            |
|AH20      |flash_address<6>    |IOB      |IO_L69N_5/VREF_5      |OUTPUT   |LVTTL      |5             |12        |SLOW     |NONE**     |         |       |LOCATED   |         |NO         |NONE            |
|AH21      |flash_address<8>    |IOB      |IO_L69P_5             |OUTPUT   |LVTTL      |5             |12        |SLOW     |NONE**     |         |       |LOCATED   |         |NO         |NONE            |
|AH22      |                    |         |GND                   |         |           |              |          |         |           |         |       |          |         |           |                |
|AH23      |tv_in_hff           |IOB      |IO_L25N_5             |INPUT    |LVTTL      |5             |          |         |           |NONE     |       |LOCATED   |         |NO         |NONE            |
|AH24      |ac97_bit_clock      |IOB      |IO_L25P_5             |INPUT    |LVTTL      |5             |          |         |           |NONE     |       |LOCATED   |         |NO         |NONE            |
|AH25      |tv_in_data_valid    |IOB      |IO_L21N_5/VREF_5      |INPUT    |LVTTL      |5             |          |         |           |NONE     |       |LOCATED   |         |NO         |NONE            |
|AH26      |tv_in_ycrcb<10>     |IOB      |IO_L04P_5/VREF_5      |INPUT    |LVTTL      |5             |          |         |           |NONE     |       |LOCATED   |         |NO         |NONE            |
|AH27      |                    |         |M0                    |         |           |              |          |         |           |         |       |          |         |           |                |
|AH28      |                    |         |GND                   |         |           |              |          |         |           |         |       |          |         |           |                |
|AH29      |ram0_data<34>       |IOB      |IO_L03P_6             |INPUT    |LVDCI_33   |6             |          |         |           |NONE     |       |LOCATED   |         |NO         |NONE            |
|AH30      |ram0_data<25>       |IOB      |IO_L03N_6/VREF_6      |INPUT    |LVDCI_33   |6             |          |         |           |NONE     |       |LOCATED   |         |NO         |NONE            |
|AH31      |ram0_data<24>       |IOB      |IO_L06P_6             |INPUT    |LVDCI_33   |6             |          |         |           |NONE     |       |LOCATED   |         |NO         |NONE            |
|AJ1       |                    |         |GND                   |         |           |              |          |         |           |         |       |          |         |           |                |
|AJ2       |                    |         |VCCAUX                |         |           |              |          |         |           |         |3.3    |          |         |           |                |
|AJ3       |                    |         |GND                   |         |           |              |          |         |           |         |       |          |         |           |                |
|AJ4       |                    |         |CCLK                  |         |           |              |          |         |           |         |       |          |         |           |                |
|AJ5       |analyzer4_data<13>  |IOB      |IO_L03P_4/D3/ALT_VRN_4|OUTPUT   |LVTTL      |4             |12        |SLOW     |NONE**     |         |       |LOCATED   |         |NO         |NONE            |
|AJ6       |vga_out_green<5>    |IOB      |IO_L23N_4             |OUTPUT   |LVTTL      |4             |12        |SLOW     |NONE**     |         |       |LOCATED   |         |NO         |NONE            |
|AJ7       |                    |         |VCCO_4                |         |           |4             |          |         |           |         |3.30   |          |         |           |                |
|AJ8       |vga_out_blank_b     |IOB      |IO_L23P_4             |OUTPUT   |LVTTL      |4             |12        |SLOW     |NONE**     |         |       |LOCATED   |         |NO         |NONE            |
|AJ9       |vga_out_sync_b      |IOB      |IO_L30N_4             |OUTPUT   |LVTTL      |4             |12        |SLOW     |NONE**     |         |       |LOCATED   |         |NO         |NONE            |
|AJ10      |vga_out_blue<1>     |IOB      |IO_L30P_4             |OUTPUT   |LVTTL      |4             |12        |SLOW     |NONE**     |         |       |LOCATED   |         |NO         |NONE            |
|AJ11      |vga_out_blue<3>     |IOB      |IO_L71N_4             |OUTPUT   |LVTTL      |4             |12        |SLOW     |NONE**     |         |       |LOCATED   |         |NO         |NONE            |
|AJ12      |flash_data<1>       |IOB      |IO_L71P_4             |INPUT    |LVTTL      |4             |          |         |           |NONE     |       |LOCATED   |         |NO         |NONE            |
|AJ13      |flash_data<0>       |IOB      |IO_L78N_4             |INPUT    |LVTTL      |4             |          |         |           |NONE     |       |LOCATED   |         |NO         |NONE            |
|AJ14      |                    |         |VCCO_4                |         |           |4             |          |         |           |         |3.30   |          |         |           |                |
|AJ15      |flash_address<23>   |IOB      |IO_L96P_4/GCLK0P      |OUTPUT   |LVTTL      |4             |12        |SLOW     |NONE**     |         |       |LOCATED   |         |NO         |NONE            |
|AJ16      |clock_feedback_in   |IOB      |IO_L96N_5/GCLK7S      |INPUT    |LVTTL      |5             |          |         |           |NONE     |       |LOCATED   |         |NO         |NONE            |
|AJ17      |flash_address<2>    |IOB      |IO_L91P_5/VREF_5      |OUTPUT   |LVTTL      |5             |12        |SLOW     |NONE**     |         |       |LOCATED   |         |NO         |NONE            |
|AJ18      |                    |         |VCCO_5                |         |           |5             |          |         |           |         |3.30   |          |         |           |                |
|AJ19      |flash_address<5>    |IOB      |IO_L73N_5             |OUTPUT   |LVTTL      |5             |12        |SLOW     |NONE**     |         |       |LOCATED   |         |NO         |NONE            |
|AJ20      |flash_address<7>    |IOB      |IO_L73P_5             |OUTPUT   |LVTTL      |5             |12        |SLOW     |NONE**     |         |       |LOCATED   |         |NO         |NONE            |
|AJ21      |flash_ce_b          |IOB      |IO_L52N_5             |OUTPUT   |LVDCI_33   |5             |          |NONE*    |NONE**     |         |       |LOCATED   |         |NO         |DRIVER          |
|AJ22      |tv_in_aff           |IOB      |IO_L52P_5             |INPUT    |LVTTL      |5             |          |         |           |NONE     |       |LOCATED   |         |NO         |NONE            |
|AJ23      |tv_in_aef           |IOB      |IO_L30N_5             |INPUT    |LVTTL      |5             |          |         |           |NONE     |       |LOCATED   |         |NO         |NONE            |
|AJ24      |ac97_sdata_in       |IOB      |IO_L30P_5             |INPUT    |LVTTL      |5             |          |         |           |NONE     |       |LOCATED   |         |NO         |NONE            |
|AJ25      |                    |         |VCCO_5                |         |           |5             |          |         |           |         |3.30   |          |         |           |                |
|AJ26      |tv_in_ycrcb<11>     |IOB      |IO_L04N_5             |INPUT    |LVTTL      |5             |          |         |           |NONE     |       |LOCATED   |         |NO         |NONE            |
|AJ27      |tv_in_iso           |IOB      |IO_L06P_5             |OUTPUT   |LVDCI_33   |5             |          |NONE*    |NONE**     |         |       |LOCATED   |         |NO         |DRIVER          |
|AJ28      |                    |         |M1                    |         |           |              |          |         |           |         |       |          |         |           |                |
|AJ29      |                    |         |GND                   |         |           |              |          |         |           |         |       |          |         |           |                |
|AJ30      |                    |         |VCCAUX                |         |           |              |          |         |           |         |3.3    |          |         |           |                |
|AJ31      |                    |         |GND                   |         |           |              |          |         |           |         |       |          |         |           |                |
|AK1       |                    |         |GND                   |         |           |              |          |         |           |         |       |          |         |           |                |
|AK2       |                    |         |GND                   |         |           |              |          |         |           |         |       |          |         |           |                |
|AK3       |analyzer4_data<14>  |IOB      |IO_L03N_4/D2/ALT_VRP_4|OUTPUT   |LVTTL      |4             |12        |SLOW     |NONE**     |         |       |LOCATED   |         |NO         |NONE            |
|AK4       |                    |DIFFS    |IO_L05N_4/VRP_4       |UNUSED   |           |4             |          |         |TERMINATION|         |       |          |         |           |                |
|AK5       |                    |DIFFM    |IO_L05P_4/VRN_4       |UNUSED   |           |4             |          |         |TERMINATION|         |       |          |         |           |                |
|AK6       |button_down         |IOB      |IO_L24N_4             |INPUT    |LVTTL      |4             |          |         |           |NONE     |       |LOCATED   |         |NO         |NONE            |
|AK7       |button_enter        |IOB      |IO_L24P_4             |INPUT    |LVTTL      |4             |          |         |           |NONE     |       |LOCATED   |         |NO         |NONE            |
|AK8       |                    |         |GND                   |         |           |              |          |         |           |         |       |          |         |           |                |
|AK9       |flash_oe_b          |IOB      |IO_L53N_4             |OUTPUT   |LVDCI_33   |4             |          |NONE*    |NONE**     |         |       |LOCATED   |         |NO         |DRIVER          |
|AK10      |flash_data<15>      |IOB      |IO_L53P_4             |INPUT    |LVTTL      |4             |          |         |           |NONE     |       |LOCATED   |         |NO         |NONE            |
|AK11      |flash_data<14>      |IOB      |IO_L72N_4             |INPUT    |LVTTL      |4             |          |         |           |NONE     |       |LOCATED   |         |NO         |NONE            |
|AK12      |flash_data<13>      |IOB      |IO_L72P_4             |INPUT    |LVTTL      |4             |          |         |           |NONE     |       |LOCATED   |         |NO         |NONE            |
|AK13      |flash_data<12>      |IOB      |IO_L78P_4             |INPUT    |LVTTL      |4             |          |         |           |NONE     |       |LOCATED   |         |NO         |NONE            |
|AK14      |flash_data<11>      |IOB      |IO_L93N_4             |INPUT    |LVTTL      |4             |          |         |           |NONE     |       |LOCATED   |         |NO         |NONE            |
|AK15      |flash_data<10>      |IOB      |IO_L93P_4             |INPUT    |LVTTL      |4             |          |         |           |NONE     |       |LOCATED   |         |NO         |NONE            |
|AK16      |                    |         |VCCAUX                |         |           |              |          |         |           |         |3.3    |          |         |           |                |
|AK17      |flash_address<10>   |IOB      |IO_L91N_5             |OUTPUT   |LVTTL      |5             |12        |SLOW     |NONE**     |         |       |LOCATED   |         |NO         |NONE            |
|AK18      |flash_reset_b       |IOB      |IO_L78N_5             |OUTPUT   |LVDCI_33   |5             |          |NONE*    |NONE**     |         |       |LOCATED   |         |NO         |DRIVER          |
|AK19      |flash_address<13>   |IOB      |IO_L78P_5             |OUTPUT   |LVTTL      |5             |12        |SLOW     |NONE**     |         |       |LOCATED   |         |NO         |NONE            |
|AK20      |flash_address<15>   |IOB      |IO_L70N_5             |OUTPUT   |LVTTL      |5             |12        |SLOW     |NONE**     |         |       |LOCATED   |         |NO         |NONE            |
|AK21      |flash_address<17>   |IOB      |IO_L70P_5             |OUTPUT   |LVTTL      |5             |12        |SLOW     |NONE**     |         |       |LOCATED   |         |NO         |NONE            |
|AK22      |flash_address<19>   |IOB      |IO_L49N_5             |OUTPUT   |LVTTL      |5             |12        |SLOW     |NONE**     |         |       |LOCATED   |         |NO         |NONE            |
|AK23      |flash_address<21>   |IOB      |IO_L49P_5             |OUTPUT   |LVTTL      |5             |12        |SLOW     |NONE**     |         |       |LOCATED   |         |NO         |NONE            |
|AK24      |                    |         |GND                   |         |           |              |          |         |           |         |       |          |         |           |                |
|AK25      |switch<2>           |IOB      |IO_L22N_5             |INPUT    |LVTTL      |5             |          |         |           |IFD      |       |LOCATED   |         |YES        |NONE            |
|AK26      |switch<0>           |IOB      |IO_L22P_5             |INPUT    |LVTTL      |5             |          |         |           |IFD      |       |LOCATED   |         |YES        |NONE            |
|AK27      |analyzer4_data<5>   |IOB      |IO_L06N_5             |OUTPUT   |LVTTL      |5             |12        |SLOW     |NONE**     |         |       |LOCATED   |         |NO         |NONE            |
|AK28      |analyzer4_data<11>  |IOB      |IO_L01N_5/RDWR_B      |OUTPUT   |LVTTL      |5             |12        |SLOW     |NONE**     |         |       |LOCATED   |         |NO         |NONE            |
|AK29      |analyzer4_data<12>  |IOB      |IO_L01P_5/CS_B        |OUTPUT   |LVTTL      |5             |12        |SLOW     |NONE**     |         |       |LOCATED   |         |NO         |NONE            |
|AK30      |                    |         |GND                   |         |           |              |          |         |           |         |       |          |         |           |                |
|AK31      |                    |         |GND                   |         |           |              |          |         |           |         |       |          |         |           |                |
|AL2       |                    |         |GND                   |         |           |              |          |         |           |         |       |          |         |           |                |
|AL3       |                    |         |GND                   |         |           |              |          |         |           |         |       |          |         |           |                |
|AL4       |button_up           |IOB      |IO_L21N_4             |INPUT    |LVTTL      |4             |          |         |           |NONE     |       |LOCATED   |         |NO         |NONE            |
|AL5       |button_left         |IOB      |IO_L21P_4/VREF_4      |INPUT    |LVTTL      |4             |          |         |           |NONE     |       |LOCATED   |         |NO         |NONE            |
|AL6       |button_right        |IOB      |IO_L29N_4             |INPUT    |LVTTL      |4             |          |         |           |NONE     |       |LOCATED   |         |NO         |NONE            |
|AL7       |                    |DIFFM    |IO_L29P_4             |UNUSED   |           |4             |          |         |           |         |       |          |         |           |                |
|AL8       |flash_we_b          |IOB      |IO_L51N_4             |OUTPUT   |LVDCI_33   |4             |          |NONE*    |NONE**     |         |       |LOCATED   |         |NO         |DRIVER          |
|AL9       |flash_sts           |IOB      |IO_L51P_4/VREF_4      |INPUT    |LVTTL      |4             |          |         |PULLUP     |NONE     |       |LOCATED   |         |NO         |NONE            |
|AL10      |flash_data<7>       |IOB      |IO_L69N_4             |INPUT    |LVTTL      |4             |          |         |           |NONE     |       |LOCATED   |         |NO         |NONE            |
|AL11      |flash_data<6>       |IOB      |IO_L69P_4/VREF_4      |INPUT    |LVTTL      |4             |          |         |           |NONE     |       |LOCATED   |         |NO         |NONE            |
|AL12      |flash_data<5>       |IOB      |IO_L75N_4             |INPUT    |LVTTL      |4             |          |         |           |NONE     |       |LOCATED   |         |NO         |NONE            |
|AL13      |flash_data<4>       |IOB      |IO_L75P_4/VREF_4      |INPUT    |LVTTL      |4             |          |         |           |NONE     |       |LOCATED   |         |NO         |NONE            |
|AL14      |flash_data<3>       |IOB      |IO_L95N_4/GCLK3S      |INPUT    |LVTTL      |4             |          |         |           |NONE     |       |LOCATED   |         |NO         |NONE            |
|AL15      |flash_data<2>       |IOB      |IO_L95P_4/GCLK2P      |INPUT    |LVTTL      |4             |          |         |           |NONE     |       |LOCATED   |         |NO         |NONE            |
|AL16      |                    |         |GND                   |         |           |              |          |         |           |         |       |          |         |           |                |
|AL17      |flash_address<9>    |IOB      |IO_L94N_5             |OUTPUT   |LVTTL      |5             |12        |SLOW     |NONE**     |         |       |LOCATED   |         |NO         |NONE            |
|AL18      |flash_address<11>   |IOB      |IO_L94P_5/VREF_5      |OUTPUT   |LVTTL      |5             |12        |SLOW     |NONE**     |         |       |LOCATED   |         |NO         |NONE            |
|AL19      |flash_address<12>   |IOB      |IO_L75N_5/VREF_5      |OUTPUT   |LVTTL      |5             |12        |SLOW     |NONE**     |         |       |LOCATED   |         |NO         |NONE            |
|AL20      |flash_address<14>   |IOB      |IO_L75P_5             |OUTPUT   |LVTTL      |5             |12        |SLOW     |NONE**     |         |       |LOCATED   |         |NO         |NONE            |
|AL21      |flash_address<16>   |IOB      |IO_L67N_5             |OUTPUT   |LVTTL      |5             |12        |SLOW     |NONE**     |         |       |LOCATED   |         |NO         |NONE            |
|AL22      |flash_address<18>   |IOB      |IO_L67P_5             |OUTPUT   |LVTTL      |5             |12        |SLOW     |NONE**     |         |       |LOCATED   |         |NO         |NONE            |
|AL23      |flash_address<20>   |IOB      |IO_L28N_5             |OUTPUT   |LVTTL      |5             |12        |SLOW     |NONE**     |         |       |LOCATED   |         |NO         |NONE            |
|AL24      |                    |DIFFM    |IO_L28P_5             |UNUSED   |           |5             |          |         |           |         |       |          |         |           |                |
|AL25      |flash_address<22>   |IOB      |IO_L27N_5/VREF_5      |OUTPUT   |LVTTL      |5             |12        |SLOW     |NONE**     |         |       |LOCATED   |         |NO         |NONE            |
|AL26      |switch<1>           |IOB      |IO_L27P_5             |INPUT    |LVTTL      |5             |          |         |           |IFD      |       |LOCATED   |         |YES        |NONE            |
|AL27      |analyzer4_data<6>   |IOB      |IO_L19N_5             |OUTPUT   |LVTTL      |5             |12        |SLOW     |NONE**     |         |       |LOCATED   |         |NO         |NONE            |
|AL28      |clock_feedback_out  |IOB      |IO_L19P_5             |OUTPUT   |LVDCI_33   |5             |          |NONE*    |NONE**     |         |       |LOCATED   |         |NO         |DRIVER          |
|AL29      |                    |         |GND                   |         |           |              |          |         |           |         |       |          |         |           |                |
|AL30      |                    |         |GND                   |         |           |              |          |         |           |         |       |          |         |           |                |
|B1        |                    |         |GND                   |         |           |              |          |         |           |         |       |          |         |           |                |
|B2        |                    |         |GND                   |         |           |              |          |         |           |         |       |          |         |           |                |
|B3        |user1<0>            |IOB      |IO_L01P_1             |OUTPUT   |LVTTL      |1             |12        |SLOW     |NONE**     |         |       |LOCATED   |         |NO         |NONE            |
|B4        |                    |         |NC                    |         |           |              |          |         |           |         |       |          |         |           |                |
|B5        |user1<2>            |IOB      |IO_L01N_1             |INPUT    |LVTTL      |1             |          |         |           |NONE     |       |LOCATED   |         |NO         |NONE            |
|B6        |user1<3>            |IOB      |IO_L19N_1             |INPUT    |LVTTL      |1             |          |         |           |NONE     |       |LOCATED   |         |NO         |NONE            |
|B7        |                    |DIFFM    |IO_L49P_1             |UNUSED   |           |1             |          |         |           |         |       |          |         |           |                |
|B8        |                    |         |GND                   |         |           |              |          |         |           |         |       |          |         |           |                |
|B9        |user3<4>            |IOB      |IO_L49N_1             |INPUT    |LVTTL      |1             |          |         |           |NONE     |       |LOCATED   |         |NO         |NONE            |
|B10       |user3<5>            |IOB      |IO_L67P_1             |INPUT    |LVTTL      |1             |          |         |           |NONE     |       |LOCATED   |         |NO         |NONE            |
|B11       |user3<6>            |IOB      |IO_L67N_1             |INPUT    |LVTTL      |1             |          |         |           |NONE     |       |LOCATED   |         |NO         |NONE            |
|B12       |user3<7>            |IOB      |IO_L71P_1             |INPUT    |LVTTL      |1             |          |         |           |NONE     |       |LOCATED   |         |NO         |NONE            |
|B13       |                    |DIFFS    |IO_L71N_1             |UNUSED   |           |1             |          |         |           |         |       |          |         |           |                |
|B14       |user1<22>           |IOB      |IO_L91P_1/VREF_1      |INPUT    |LVTTL      |1             |          |         |           |NONE     |       |LOCATED   |         |NO         |NONE            |
|B15       |user1<23>           |IOB      |IO_L91N_1             |INPUT    |LVTTL      |1             |          |         |           |NONE     |       |LOCATED   |         |NO         |NONE            |
|B16       |                    |         |VCCAUX                |         |           |              |          |         |           |         |3.3    |          |         |           |                |
|B17       |                    |DIFFM    |IO_L93P_0             |UNUSED   |           |0             |          |         |           |         |       |          |         |           |                |
|B18       |user4<8>            |IOB      |IO_L93N_0             |INPUT    |LVTTL      |0             |          |         |           |NONE     |       |LOCATED   |         |NO         |NONE            |
|B19       |user4<9>            |IOB      |IO_L73P_0             |INPUT    |LVTTL      |0             |          |         |           |NONE     |       |LOCATED   |         |NO         |NONE            |
|B20       |user4<24>           |IOB      |IO_L73N_0             |INPUT    |LVTTL      |0             |          |         |           |NONE     |       |LOCATED   |         |NO         |NONE            |
|B21       |user4<25>           |IOB      |IO_L54P_0             |INPUT    |LVTTL      |0             |          |         |           |NONE     |       |LOCATED   |         |NO         |NONE            |
|B22       |user4<26>           |IOB      |IO_L54N_0             |INPUT    |LVTTL      |0             |          |         |           |NONE     |       |LOCATED   |         |NO         |NONE            |
|B23       |user4<27>           |IOB      |IO_L30P_0             |INPUT    |LVTTL      |0             |          |         |           |NONE     |       |LOCATED   |         |NO         |NONE            |
|B24       |                    |         |GND                   |         |           |              |          |         |           |         |       |          |         |           |                |
|B25       |user2<29>           |IOB      |IO_L30N_0             |INPUT    |LVTTL      |0             |          |         |           |NONE     |       |LOCATED   |         |NO         |NONE            |
|B26       |user2<30>           |IOB      |IO_L21P_0/VREF_0      |INPUT    |LVTTL      |0             |          |         |           |NONE     |       |LOCATED   |         |NO         |NONE            |
|B27       |user2<31>           |IOB      |IO_L21N_0             |INPUT    |LVTTL      |0             |          |         |           |NONE     |       |LOCATED   |         |NO         |NONE            |
|B28       |                    |         |DXP                   |         |           |              |          |         |           |         |       |          |         |           |                |
|B29       |                    |DIFFS    |IO_L03N_0/VRP_0       |UNUSED   |           |0             |          |         |           |         |       |          |         |           |                |
|B30       |                    |         |GND                   |         |           |              |          |         |           |         |       |          |         |           |                |
|B31       |                    |         |GND                   |         |           |              |          |         |           |         |       |          |         |           |                |
|C1        |                    |         |GND                   |         |           |              |          |         |           |         |       |          |         |           |                |
|C2        |                    |         |VCCAUX                |         |           |              |          |         |           |         |3.3    |          |         |           |                |
|C3        |                    |         |GND                   |         |           |              |          |         |           |         |       |          |         |           |                |
|C4        |                    |         |TDO                   |         |           |              |          |         |           |         |       |          |         |           |                |
|C5        |user1<1>            |IOB      |IO_L19P_1             |INPUT    |LVTTL      |1             |          |         |           |NONE     |       |LOCATED   |         |NO         |NONE            |
|C6        |user1<9>            |IOB      |IO_L06N_1             |INPUT    |LVTTL      |1             |          |         |           |NONE     |       |LOCATED   |         |NO         |NONE            |
|C7        |                    |         |VCCO_1                |         |           |1             |          |         |           |         |3.30   |          |         |           |                |
|C8        |user1<10>           |IOB      |IO_L25P_1             |INPUT    |LVTTL      |1             |          |         |           |NONE     |       |LOCATED   |         |NO         |NONE            |
|C9        |user1<11>           |IOB      |IO_L25N_1             |INPUT    |LVTTL      |1             |          |         |           |NONE     |       |LOCATED   |         |NO         |NONE            |
|C10       |user1<12>           |IOB      |IO_L50P_1             |INPUT    |LVTTL      |1             |          |         |           |NONE     |       |LOCATED   |         |NO         |NONE            |
|C11       |user1<13>           |IOB      |IO_L50N_1             |INPUT    |LVTTL      |1             |          |         |           |NONE     |       |LOCATED   |         |NO         |NONE            |
|C12       |user1<14>           |IOB      |IO_L70P_1             |INPUT    |LVTTL      |1             |          |         |           |NONE     |       |LOCATED   |         |NO         |NONE            |
|C13       |user1<15>           |IOB      |IO_L70N_1             |INPUT    |LVTTL      |1             |          |         |           |NONE     |       |LOCATED   |         |NO         |NONE            |
|C14       |                    |         |VCCO_1                |         |           |1             |          |         |           |         |3.30   |          |         |           |                |
|C15       |clock2              |IOB      |IO_L96P_1/GCLK2S      |INPUT    |LVTTL      |1             |          |         |           |NONE     |       |LOCATED   |         |NO         |NONE            |
|C16       |clock_27mhz         |IOB      |IO_L96N_1/GCLK3P      |INPUT    |LVTTL      |1             |          |         |           |NONE     |       |LOCATED   |         |NO         |NONE            |
|C17       |                    |DIFFM    |IO_L78P_0             |UNUSED   |           |0             |          |         |           |         |       |          |         |           |                |
|C18       |                    |         |VCCO_0                |         |           |0             |          |         |           |         |3.30   |          |         |           |                |
|C19       |user4<16>           |IOB      |IO_L78N_0             |INPUT    |LVTTL      |0             |          |         |           |NONE     |       |LOCATED   |         |NO         |NONE            |
|C20       |user4<17>           |IOB      |IO_L72P_0             |INPUT    |LVTTL      |0             |          |         |           |NONE     |       |LOCATED   |         |NO         |NONE            |
|C21       |user4<18>           |IOB      |IO_L72N_0             |INPUT    |LVTTL      |0             |          |         |           |NONE     |       |LOCATED   |         |NO         |NONE            |
|C22       |user4<19>           |IOB      |IO_L49P_0             |INPUT    |LVTTL      |0             |          |         |           |NONE     |       |LOCATED   |         |NO         |NONE            |
|C23       |user4<20>           |IOB      |IO_L49N_0             |INPUT    |LVTTL      |0             |          |         |           |NONE     |       |LOCATED   |         |NO         |NONE            |
|C24       |user2<21>           |IOB      |IO_L23P_0             |INPUT    |LVTTL      |0             |          |         |           |NONE     |       |LOCATED   |         |NO         |NONE            |
|C25       |                    |         |VCCO_0                |         |           |0             |          |         |           |         |3.30   |          |         |           |                |
|C26       |user4<22>           |IOB      |IO_L23N_0             |INPUT    |LVTTL      |0             |          |         |           |NONE     |       |LOCATED   |         |NO         |NONE            |
|C27       |                    |DIFFM    |IO_L03P_0/VRN_0       |UNUSED   |           |0             |          |         |           |         |       |          |         |           |                |
|C28       |                    |         |TDI                   |         |           |              |          |         |           |         |       |          |         |           |                |
|C29       |                    |         |GND                   |         |           |              |          |         |           |         |       |          |         |           |                |
|C30       |                    |         |VCCAUX                |         |           |              |          |         |           |         |3.3    |          |         |           |                |
|C31       |                    |         |GND                   |         |           |              |          |         |           |         |       |          |         |           |                |
|D1        |daughtercard<11>    |IOB      |IO_L21N_2             |INPUT    |LVTTL      |2             |          |         |           |NONE     |       |LOCATED   |         |NO         |NONE            |
|D2        |daughtercard<12>    |IOB      |IO_L05N_2             |INPUT    |LVTTL      |2             |          |         |           |NONE     |       |LOCATED   |         |NO         |NONE            |
|D3        |daughtercard<21>    |IOB      |IO_L03N_2             |INPUT    |LVTTL      |2             |          |         |           |NONE     |       |LOCATED   |         |NO         |NONE            |
|D4        |                    |         |GND                   |         |           |              |          |         |           |         |       |          |         |           |                |
|D5        |                    |         |VBATT                 |         |           |              |          |         |           |         |       |          |         |           |                |
|D6        |user3<8>            |IOB      |IO_L06P_1             |INPUT    |LVTTL      |1             |          |         |           |NONE     |       |LOCATED   |         |NO         |NONE            |
|D7        |user3<9>            |IOB      |IO_L04N_1             |INPUT    |LVTTL      |1             |          |         |           |NONE     |       |LOCATED   |         |NO         |NONE            |
|D8        |user3<10>           |IOB      |IO_L27P_1             |INPUT    |LVTTL      |1             |          |         |           |NONE     |       |LOCATED   |         |NO         |NONE            |
|D9        |user3<11>           |IOB      |IO_L27N_1/VREF_1      |INPUT    |LVTTL      |1             |          |         |           |NONE     |       |LOCATED   |         |NO         |NONE            |
|D10       |                    |         |GND                   |         |           |              |          |         |           |         |       |          |         |           |                |
|D11       |user3<12>           |IOB      |IO_L68P_1             |INPUT    |LVTTL      |1             |          |         |           |NONE     |       |LOCATED   |         |NO         |NONE            |
|D12       |user3<13>           |IOB      |IO_L68N_1             |INPUT    |LVTTL      |1             |          |         |           |NONE     |       |LOCATED   |         |NO         |NONE            |
|D13       |user3<14>           |IOB      |IO_L76P_1             |INPUT    |LVTTL      |1             |          |         |           |NONE     |       |LOCATED   |         |NO         |NONE            |
|D14       |user3<15>           |IOB      |IO_L76N_1             |INPUT    |LVTTL      |1             |          |         |           |NONE     |       |LOCATED   |         |NO         |NONE            |
|D15       |                    |DIFFS    |IO_L78N_1             |UNUSED   |           |1             |          |         |           |         |       |          |         |           |                |
|D16       |                    |         |GND                   |         |           |              |          |         |           |         |       |          |         |           |                |
|D17       |                    |DIFFM    |IO_L75P_0/VREF_0      |UNUSED   |           |0             |          |         |           |         |       |          |         |           |                |
|D18       |user2<16>           |IOB      |IO_L77P_0             |INPUT    |LVTTL      |0             |          |         |           |NONE     |       |LOCATED   |         |NO         |NONE            |
|D19       |user2<17>           |IOB      |IO_L77N_0             |INPUT    |LVTTL      |0             |          |         |           |NONE     |       |LOCATED   |         |NO         |NONE            |
|D20       |user2<18>           |IOB      |IO_L67P_0             |INPUT    |LVTTL      |0             |          |         |           |NONE     |       |LOCATED   |         |NO         |NONE            |
|D21       |user2<19>           |IOB      |IO_L67N_0             |INPUT    |LVTTL      |0             |          |         |           |NONE     |       |LOCATED   |         |NO         |NONE            |
|D22       |                    |         |GND                   |         |           |              |          |         |           |         |       |          |         |           |                |
|D23       |user2<20>           |IOB      |IO_L24P_0             |INPUT    |LVTTL      |0             |          |         |           |NONE     |       |LOCATED   |         |NO         |NONE            |
|D24       |user4<21>           |IOB      |IO_L24N_0             |INPUT    |LVTTL      |0             |          |         |           |NONE     |       |LOCATED   |         |NO         |NONE            |
|D25       |user2<22>           |IOB      |IO_L05P_0             |INPUT    |LVTTL      |0             |          |         |           |NONE     |       |LOCATED   |         |NO         |NONE            |
|D26       |user2<23>           |IOB      |IO_L05N_0             |INPUT    |LVTTL      |0             |          |         |           |NONE     |       |LOCATED   |         |NO         |NONE            |
|D27       |                    |         |PROG_B                |         |           |              |          |         |           |         |       |          |         |           |                |
|D28       |                    |         |GND                   |         |           |              |          |         |           |         |       |          |         |           |                |
|D29       |systemace_irq       |IOB      |IO_L01N_7             |INPUT    |LVTTL      |7             |          |         |           |NONE     |       |LOCATED   |         |NO         |NONE            |
|D30       |                    |DIFFM    |IO_L01P_7             |UNUSED   |           |7             |          |         |           |         |       |          |         |           |                |
|D31       |                    |DIFFS    |IO_L19N_7             |UNUSED   |           |7             |          |         |           |         |       |          |         |           |                |
|E1        |daughtercard<9>     |IOB      |IO_L21P_2/VREF_2      |INPUT    |LVTTL      |2             |          |         |           |NONE     |       |LOCATED   |         |NO         |NONE            |
|E2        |daughtercard<10>    |IOB      |IO_L23N_2             |INPUT    |LVTTL      |2             |          |         |           |NONE     |       |LOCATED   |         |NO         |NONE            |
|E3        |daughtercard<19>    |IOB      |IO_L05P_2             |INPUT    |LVTTL      |2             |          |         |           |NONE     |       |LOCATED   |         |NO         |NONE            |
|E4        |daughtercard<20>    |IOB      |IO_L03P_2/VREF_2      |INPUT    |LVTTL      |2             |          |         |           |NONE     |       |LOCATED   |         |NO         |NONE            |
|E5        |                    |         |GND                   |         |           |              |          |         |           |         |       |          |         |           |                |
|E6        |user1<8>            |IOB      |IO_L04P_1/VREF_1      |INPUT    |LVTTL      |1             |          |         |           |NONE     |       |LOCATED   |         |NO         |NONE            |
|E7        |                    |DIFFM    |IO_L03P_1/VRN_1       |UNUSED   |           |1             |          |         |           |         |       |          |         |           |                |
|E8        |                    |DIFFS    |IO_L03N_1/VRP_1       |UNUSED   |           |1             |          |         |           |         |       |          |         |           |                |
|E9        |user1<18>           |IOB      |IO_L24P_1             |INPUT    |LVTTL      |1             |          |         |           |NONE     |       |LOCATED   |         |NO         |NONE            |
|E10       |user3<18>           |IOB      |IO_L24N_1             |INPUT    |LVTTL      |1             |          |         |           |NONE     |       |LOCATED   |         |NO         |NONE            |
|E11       |user1<19>           |IOB      |IO_L54P_1             |INPUT    |LVTTL      |1             |          |         |           |NONE     |       |LOCATED   |         |NO         |NONE            |
|E12       |user3<19>           |IOB      |IO_L54N_1             |INPUT    |LVTTL      |1             |          |         |           |NONE     |       |LOCATED   |         |NO         |NONE            |
|E13       |user1<20>           |IOB      |IO_L75P_1             |INPUT    |LVTTL      |1             |          |         |           |NONE     |       |LOCATED   |         |NO         |NONE            |
|E14       |user3<20>           |IOB      |IO_L75N_1/VREF_1      |INPUT    |LVTTL      |1             |          |         |           |NONE     |       |LOCATED   |         |NO         |NONE            |
|E15       |user3<21>           |IOB      |IO_L78P_1             |INPUT    |LVTTL      |1             |          |         |           |NONE     |       |LOCATED   |         |NO         |NONE            |
|E16       |user2<10>           |IOB      |IO_L95P_0/GCLK6S      |INPUT    |LVTTL      |0             |          |         |           |NONE     |       |LOCATED   |         |NO         |NONE            |
|E17       |user4<10>           |IOB      |IO_L95N_0/GCLK7P      |INPUT    |LVTTL      |0             |          |         |           |NONE     |       |LOCATED   |         |NO         |NONE            |
|E18       |user2<11>           |IOB      |IO_L75N_0             |INPUT    |LVTTL      |0             |          |         |           |NONE     |       |LOCATED   |         |NO         |NONE            |
|E19       |user4<11>           |IOB      |IO_L53P_0             |INPUT    |LVTTL      |0             |          |         |           |NONE     |       |LOCATED   |         |NO         |NONE            |
|E20       |user2<12>           |IOB      |IO_L53N_0             |INPUT    |LVTTL      |0             |          |         |           |NONE     |       |LOCATED   |         |NO         |NONE            |
|E21       |user4<12>           |IOB      |IO_L50P_0             |INPUT    |LVTTL      |0             |          |         |           |NONE     |       |LOCATED   |         |NO         |NONE            |
|E22       |user2<13>           |IOB      |IO_L50N_0             |INPUT    |LVTTL      |0             |          |         |           |NONE     |       |LOCATED   |         |NO         |NONE            |
|E23       |user4<13>           |IOB      |IO_L25P_0             |INPUT    |LVTTL      |0             |          |         |           |NONE     |       |LOCATED   |         |NO         |NONE            |
|E24       |user4<14>           |IOB      |IO_L25N_0             |INPUT    |LVTTL      |0             |          |         |           |NONE     |       |LOCATED   |         |NO         |NONE            |
|E25       |user4<23>           |IOB      |IO_L02P_0             |INPUT    |LVTTL      |0             |          |         |           |NONE     |       |LOCATED   |         |NO         |NONE            |
|E26       |                    |         |HSWAP_EN              |         |           |              |          |         |           |         |       |          |         |           |                |
|E27       |                    |         |GND                   |         |           |              |          |         |           |         |       |          |         |           |                |
|E28       |systemace_ce_b      |IOB      |IO_L06N_7             |OUTPUT   |LVTTL      |7             |12        |SLOW     |NONE**     |         |       |LOCATED   |         |NO         |NONE            |
|E29       |systemace_address<6>|IOB      |IO_L04N_7             |OUTPUT   |LVTTL      |7             |12        |SLOW     |NONE**     |         |       |LOCATED   |         |NO         |NONE            |
|E30       |                    |DIFFS    |IO_L24N_7             |UNUSED   |           |7             |          |         |           |         |       |          |         |           |                |
|E31       |                    |DIFFM    |IO_L19P_7             |UNUSED   |           |7             |          |         |           |         |       |          |         |           |                |
|F1        |analyzer2_clock     |IOB      |IO_L43N_2             |OUTPUT   |LVTTL      |2             |12        |SLOW     |NONE**     |         |       |LOCATED   |         |NO         |NONE            |
|F2        |analyzer2_data<15>  |IOB      |IO_L23P_2             |OUTPUT   |LVTTL      |2             |12        |SLOW     |NONE**     |         |       |LOCATED   |         |NO         |NONE            |
|F3        |daughtercard<17>    |IOB      |IO_L06P_2             |INPUT    |LVTTL      |2             |          |         |           |NONE     |       |LOCATED   |         |NO         |NONE            |
|F4        |daughtercard<18>    |IOB      |IO_L06N_2             |INPUT    |LVTTL      |2             |          |         |           |NONE     |       |LOCATED   |         |NO         |NONE            |
|F5        |daughtercard<8>     |IOB      |IO_L01N_2             |INPUT    |LVTTL      |2             |          |         |           |NONE     |       |LOCATED   |         |NO         |NONE            |
|F6        |                    |         |GND                   |         |           |              |          |         |           |         |       |          |         |           |                |
|F7        |user1<16>           |IOB      |IO_L02P_1             |INPUT    |LVTTL      |1             |          |         |           |NONE     |       |LOCATED   |         |NO         |NONE            |
|F8        |user1<17>           |IOB      |IO_L02N_1             |INPUT    |LVTTL      |1             |          |         |           |NONE     |       |LOCATED   |         |NO         |NONE            |
|F9        |user3<17>           |IOB      |IO_L30P_1             |INPUT    |LVTTL      |1             |          |         |           |NONE     |       |LOCATED   |         |NO         |NONE            |
|F10       |                    |         |VCCO_1                |         |           |1             |          |         |           |         |3.30   |          |         |           |                |
|F11       |user3<26>           |IOB      |IO_L30N_1             |INPUT    |LVTTL      |1             |          |         |           |NONE     |       |LOCATED   |         |NO         |NONE            |
|F12       |user1<27>           |IOB      |IO_L73P_1             |INPUT    |LVTTL      |1             |          |         |           |NONE     |       |LOCATED   |         |NO         |NONE            |
|F13       |user3<27>           |IOB      |IO_L73N_1             |INPUT    |LVTTL      |1             |          |         |           |NONE     |       |LOCATED   |         |NO         |NONE            |
|F14       |user1<28>           |IOB      |IO_L93P_1             |INPUT    |LVTTL      |1             |          |         |           |NONE     |       |LOCATED   |         |NO         |NONE            |
|F15       |user1<21>           |IOB      |IO_L93N_1             |INPUT    |LVTTL      |1             |          |         |           |NONE     |       |LOCATED   |         |NO         |NONE            |
|F16       |user4<2>            |IOB      |IO_L92P_0             |INPUT    |LVTTL      |0             |          |         |           |NONE     |       |LOCATED   |         |NO         |NONE            |
|F17       |user2<3>            |IOB      |IO_L92N_0             |INPUT    |LVTTL      |0             |          |         |           |NONE     |       |LOCATED   |         |NO         |NONE            |
|F18       |user4<3>            |IOB      |IO_L69P_0/VREF_0      |INPUT    |LVTTL      |0             |          |         |           |NONE     |       |LOCATED   |         |NO         |NONE            |
|F19       |user2<4>            |IOB      |IO_L69N_0             |INPUT    |LVTTL      |0             |          |         |           |NONE     |       |LOCATED   |         |NO         |NONE            |
|F20       |user4<4>            |IOB      |IO_L51P_0/VREF_0      |INPUT    |LVTTL      |0             |          |         |           |NONE     |       |LOCATED   |         |NO         |NONE            |
|F21       |user2<5>            |IOB      |IO_L51N_0             |INPUT    |LVTTL      |0             |          |         |           |NONE     |       |LOCATED   |         |NO         |NONE            |
|F22       |                    |         |VCCO_0                |         |           |0             |          |         |           |         |3.30   |          |         |           |                |
|F23       |user2<14>           |IOB      |IO_L04P_0             |INPUT    |LVTTL      |0             |          |         |           |NONE     |       |LOCATED   |         |NO         |NONE            |
|F24       |user2<15>           |IOB      |IO_L04N_0/VREF_0      |INPUT    |LVTTL      |0             |          |         |           |NONE     |       |LOCATED   |         |NO         |NONE            |
|F25       |                    |         |DXN                   |         |           |              |          |         |           |         |       |          |         |           |                |
|F26       |                    |         |GND                   |         |           |              |          |         |           |         |       |          |         |           |                |
|F27       |                    |DIFFS    |IO_L02N_7/VRP_7       |UNUSED   |           |7             |          |         |TERMINATION|         |       |          |         |           |                |
|F28       |systemace_address<5>|IOB      |IO_L06P_7             |OUTPUT   |LVTTL      |7             |12        |SLOW     |NONE**     |         |       |LOCATED   |         |NO         |NONE            |
|F29       |systemace_data<15>  |IOB      |IO_L04P_7             |INPUT    |LVTTL      |7             |          |         |           |NONE     |       |LOCATED   |         |NO         |NONE            |
|F30       |                    |DIFFM    |IO_L24P_7             |UNUSED   |           |7             |          |         |           |         |       |          |         |           |                |
|F31       |                    |DIFFS    |IO_L25N_7             |UNUSED   |           |7             |          |         |           |         |       |          |         |           |                |
|G1        |analyzer1_data<15>  |IOB      |IO_L43P_2             |OUTPUT   |LVTTL      |2             |12        |SLOW     |NONE**     |         |       |LOCATED   |         |NO         |NONE            |
|G2        |analyzer1_clock     |IOB      |IO_L45N_2             |OUTPUT   |LVTTL      |2             |12        |SLOW     |NONE**     |         |       |LOCATED   |         |NO         |NONE            |
|G3        |                    |         |VCCO_2                |         |           |2             |          |         |           |         |3.30   |          |         |           |                |
|G4        |daughtercard<16>    |IOB      |IO_L01P_2             |INPUT    |LVTTL      |2             |          |         |           |NONE     |       |LOCATED   |         |NO         |NONE            |
|G5        |daughtercard<7>     |IOB      |IO_L22N_2             |INPUT    |LVTTL      |2             |          |         |           |NONE     |       |LOCATED   |         |NO         |NONE            |
|G6        |                    |DIFFS    |IO_L02N_2/VRP_2       |UNUSED   |           |2             |          |         |TERMINATION|         |       |          |         |           |                |
|G7        |                    |         |GND                   |         |           |              |          |         |           |         |       |          |         |           |                |
|G8        |user3<16>           |IOB      |IO_L05P_1             |INPUT    |LVTTL      |1             |          |         |           |NONE     |       |LOCATED   |         |NO         |NONE            |
|G9        |user1<25>           |IOB      |IO_L20P_1             |INPUT    |LVTTL      |1             |          |         |           |NONE     |       |LOCATED   |         |NO         |NONE            |
|G10       |user3<25>           |IOB      |IO_L20N_1             |INPUT    |LVTTL      |1             |          |         |           |NONE     |       |LOCATED   |         |NO         |NONE            |
|G11       |                    |DIFFM    |IO_L52P_1             |UNUSED   |           |1             |          |         |           |         |       |          |         |           |                |
|G12       |user3<31>           |IOB      |IO_L52N_1             |INPUT    |LVTTL      |1             |          |         |           |NONE     |       |LOCATED   |         |NO         |NONE            |
|G13       |                    |         |GND                   |         |           |              |          |         |           |         |       |          |         |           |                |
|G14       |user3<28>           |IOB      |IO_L92P_1             |INPUT    |LVTTL      |1             |          |         |           |NONE     |       |LOCATED   |         |NO         |NONE            |
|G15       |user1<29>           |IOB      |IO_L92N_1             |INPUT    |LVTTL      |1             |          |         |           |NONE     |       |LOCATED   |         |NO         |NONE            |
|G16       |                    |         |GND                   |         |           |              |          |         |           |         |       |          |         |           |                |
|G17       |user4<0>            |IOB      |IO_L74P_0             |INPUT    |LVTTL      |0             |          |         |           |NONE     |       |LOCATED   |         |NO         |NONE            |
|G18       |user4<1>            |IOB      |IO_L74N_0             |INPUT    |LVTTL      |0             |          |         |           |NONE     |       |LOCATED   |         |NO         |NONE            |
|G19       |                    |         |GND                   |         |           |              |          |         |           |         |       |          |         |           |                |
|G20       |user2<1>            |IOB      |IO_L26P_0             |INPUT    |LVTTL      |0             |          |         |           |NONE     |       |LOCATED   |         |NO         |NONE            |
|G21       |user4<5>            |IOB      |IO_L26N_0             |INPUT    |LVTTL      |0             |          |         |           |NONE     |       |LOCATED   |         |NO         |NONE            |
|G22       |user2<6>            |IOB      |IO_L20P_0             |INPUT    |LVTTL      |0             |          |         |           |NONE     |       |LOCATED   |         |NO         |NONE            |
|G23       |user4<6>            |IOB      |IO_L20N_0             |INPUT    |LVTTL      |0             |          |         |           |NONE     |       |LOCATED   |         |NO         |NONE            |
|G24       |user4<15>           |IOB      |IO_L02N_0             |INPUT    |LVTTL      |0             |          |         |           |NONE     |       |LOCATED   |         |NO         |NONE            |
|G25       |                    |         |GND                   |         |           |              |          |         |           |         |       |          |         |           |                |
|G26       |                    |DIFFM    |IO_L02P_7/VRN_7       |UNUSED   |           |7             |          |         |TERMINATION|         |       |          |         |           |                |
|G27       |tv_out_reset_b      |IOB      |IO_L21N_7             |OUTPUT   |LVDCI_33   |7             |          |NONE*    |NONE**     |         |       |LOCATED   |         |NO         |DRIVER          |
|G28       |systemace_data<14>  |IOB      |IO_L22N_7             |INPUT    |LVTTL      |7             |          |         |           |NONE     |       |LOCATED   |         |NO         |NONE            |
|G29       |                    |         |VCCO_7                |         |           |7             |          |         |           |         |3.30   |          |         |           |                |
|G30       |                    |DIFFS    |IO_L44N_7             |UNUSED   |           |7             |          |         |           |         |       |          |         |           |                |
|G31       |                    |DIFFM    |IO_L25P_7             |UNUSED   |           |7             |          |         |           |         |       |          |         |           |                |
|H1        |daughtercard<42>    |IOB      |IO_L49N_2             |INPUT    |LVTTL      |2             |          |         |           |NONE     |       |LOCATED   |         |NO         |NONE            |
|H2        |                    |         |GND                   |         |           |              |          |         |           |         |       |          |         |           |                |
|H3        |analyzer1_data<14>  |IOB      |IO_L46N_2             |OUTPUT   |LVTTL      |2             |12        |SLOW     |NONE**     |         |       |LOCATED   |         |NO         |NONE            |
|H4        |daughtercard<15>    |IOB      |IO_L24N_2             |INPUT    |LVTTL      |2             |          |         |           |NONE     |       |LOCATED   |         |NO         |NONE            |
|H5        |daughtercard<6>     |IOB      |IO_L22P_2             |INPUT    |LVTTL      |2             |          |         |           |NONE     |       |LOCATED   |         |NO         |NONE            |
|H6        |                    |DIFFM    |IO_L02P_2/VRN_2       |UNUSED   |           |2             |          |         |TERMINATION|         |       |          |         |           |                |
|H7        |daughtercard<3>     |IOB      |IO_L20N_2             |INPUT    |LVTTL      |2             |          |         |           |NONE     |       |LOCATED   |         |NO         |NONE            |
|H8        |                    |         |GND                   |         |           |              |          |         |           |         |       |          |         |           |                |
|H9        |user1<24>           |IOB      |IO_L05N_1             |INPUT    |LVTTL      |1             |          |         |           |NONE     |       |LOCATED   |         |NO         |NONE            |
|H10       |user3<24>           |IOB      |IO_L23P_1             |INPUT    |LVTTL      |1             |          |         |           |NONE     |       |LOCATED   |         |NO         |NONE            |
|H11       |user1<26>           |IOB      |IO_L23N_1             |INPUT    |LVTTL      |1             |          |         |           |NONE     |       |LOCATED   |         |NO         |NONE            |
|H12       |                    |DIFFM    |IO_L69P_1             |UNUSED   |           |1             |          |         |           |         |       |          |         |           |                |
|H13       |user3<30>           |IOB      |IO_L69N_1/VREF_1      |INPUT    |LVTTL      |1             |          |         |           |NONE     |       |LOCATED   |         |NO         |NONE            |
|H14       |                    |         |VCCO_1                |         |           |1             |          |         |           |         |3.30   |          |         |           |                |
|H15       |                    |DIFFM    |IO_L95P_1/GCLK0S      |UNUSED   |           |1             |          |         |           |         |       |          |         |           |                |
|H16       |clock1              |IOB      |IO_L95N_1/GCLK1P      |INPUT    |LVTTL      |1             |          |         |           |NONE     |       |LOCATED   |         |NO         |NONE            |
|H17       |                    |DIFFM    |IO_L71P_0             |UNUSED   |           |0             |          |         |           |         |       |          |         |           |                |
|H18       |                    |         |VCCO_0                |         |           |0             |          |         |           |         |3.30   |          |         |           |                |
|H19       |user2<2>            |IOB      |IO_L71N_0             |INPUT    |LVTTL      |0             |          |         |           |NONE     |       |LOCATED   |         |NO         |NONE            |
|H20       |                    |DIFFM    |IO_L29P_0             |UNUSED   |           |0             |          |         |           |         |       |          |         |           |                |
|H21       |user2<0>            |IOB      |IO_L29N_0             |INPUT    |LVTTL      |0             |          |         |           |NONE     |       |LOCATED   |         |NO         |NONE            |
|H22       |user2<7>            |IOB      |IO_L01P_0             |INPUT    |LVTTL      |0             |          |         |           |NONE     |       |LOCATED   |         |NO         |NONE            |
|H23       |user4<7>            |IOB      |IO_L01N_0             |INPUT    |LVTTL      |0             |          |         |           |NONE     |       |LOCATED   |         |NO         |NONE            |
|H24       |                    |         |GND                   |         |           |              |          |         |           |         |       |          |         |           |                |
|H25       |tv_out_blank_b      |IOB      |IO_L03N_7             |OUTPUT   |LVDCI_33   |7             |          |NONE*    |NONE**     |         |       |LOCATED   |         |NO         |DRIVER          |
|H26       |tv_out_ycrcb<6>     |IOB      |IO_L03P_7/VREF_7      |OUTPUT   |LVDCI_33   |7             |          |NONE*    |NONE**     |         |       |LOCATED   |         |NO         |DRIVER          |
|H27       |tv_out_i2c_data     |IOB      |IO_L21P_7/VREF_7      |OUTPUT   |LVDCI_33   |7             |          |NONE*    |NONE**     |         |       |LOCATED   |         |NO         |DRIVER          |
|H28       |systemace_data<12>  |IOB      |IO_L22P_7             |INPUT    |LVTTL      |7             |          |         |           |NONE     |       |LOCATED   |         |NO         |NONE            |
|H29       |systemace_data<13>  |IOB      |IO_L46N_7             |INPUT    |LVTTL      |7             |          |         |           |NONE     |       |LOCATED   |         |NO         |NONE            |
|H30       |                    |         |GND                   |         |           |              |          |         |           |         |       |          |         |           |                |
|H31       |systemace_address<4>|IOB      |IO_L47N_7             |OUTPUT   |LVTTL      |7             |12        |SLOW     |NONE**     |         |       |LOCATED   |         |NO         |NONE            |
|J1        |daughtercard<40>    |IOB      |IO_L49P_2             |INPUT    |LVTTL      |2             |          |         |           |NONE     |       |LOCATED   |         |NO         |NONE            |
|J2        |daughtercard<41>    |IOB      |IO_L45P_2/VREF_2      |INPUT    |LVTTL      |2             |          |         |           |NONE     |       |LOCATED   |         |NO         |NONE            |
|J3        |daughtercard<14>    |IOB      |IO_L46P_2             |INPUT    |LVTTL      |2             |          |         |           |NONE     |       |LOCATED   |         |NO         |NONE            |
|J4        |daughtercard<13>    |IOB      |IO_L24P_2             |INPUT    |LVTTL      |2             |          |         |           |NONE     |       |LOCATED   |         |NO         |NONE            |
|J5        |daughtercard<5>     |IOB      |IO_L48N_2             |INPUT    |LVTTL      |2             |          |         |           |NONE     |       |LOCATED   |         |NO         |NONE            |
|J6        |daughtercard<1>     |IOB      |IO_L47N_2             |INPUT    |LVTTL      |2             |          |         |           |NONE     |       |LOCATED   |         |NO         |NONE            |
|J7        |daughtercard<0>     |IOB      |IO_L27N_2             |INPUT    |LVTTL      |2             |          |         |           |NONE     |       |LOCATED   |         |NO         |NONE            |
|J8        |daughtercard<2>     |IOB      |IO_L20P_2             |INPUT    |LVTTL      |2             |          |         |           |NONE     |       |LOCATED   |         |NO         |NONE            |
|J9        |                    |         |GND                   |         |           |              |          |         |           |         |       |          |         |           |                |
|J10       |                    |         |TMS                   |         |           |              |          |         |           |         |       |          |         |           |                |
|J11       |                    |DIFFM    |IO_L26P_1             |UNUSED   |           |1             |          |         |           |         |       |          |         |           |                |
|J12       |                    |DIFFS    |IO_L26N_1             |UNUSED   |           |1             |          |         |           |         |       |          |         |           |                |
|J13       |user3<29>           |IOB      |IO_L72P_1             |INPUT    |LVTTL      |1             |          |         |           |NONE     |       |LOCATED   |         |NO         |NONE            |
|J14       |user1<30>           |IOB      |IO_L72N_1             |INPUT    |LVTTL      |1             |          |         |           |NONE     |       |LOCATED   |         |NO         |NONE            |
|J15       |user1<31>           |IOB      |IO_L77N_1             |INPUT    |LVTTL      |1             |          |         |           |NONE     |       |LOCATED   |         |NO         |NONE            |
|J16       |                    |DIFFM    |IO_L94P_0             |UNUSED   |           |0             |          |         |           |         |       |          |         |           |                |
|J17       |                    |DIFFS    |IO_L94N_0/VREF_0      |UNUSED   |           |0             |          |         |           |         |       |          |         |           |                |
|J18       |                    |DIFFM    |IO_L91P_0             |UNUSED   |           |0             |          |         |           |         |       |          |         |           |                |
|J19       |                    |DIFFM    |IO_L68P_0             |UNUSED   |           |0             |          |         |           |         |       |          |         |           |                |
|J20       |                    |DIFFS    |IO_L68N_0             |UNUSED   |           |0             |          |         |           |         |       |          |         |           |                |
|J21       |                    |DIFFM    |IO_L19P_0             |UNUSED   |           |0             |          |         |           |         |       |          |         |           |                |
|J22       |                    |DIFFS    |IO_L19N_0             |UNUSED   |           |0             |          |         |           |         |       |          |         |           |                |
|J23       |                    |         |GND                   |         |           |              |          |         |           |         |       |          |         |           |                |
|J24       |analyzer3_clock     |IOB      |IO_L20N_7             |OUTPUT   |LVTTL      |7             |12        |SLOW     |NONE**     |         |       |LOCATED   |         |NO         |NONE            |
|J25       |tv_out_pal_ntsc     |IOB      |IO_L23N_7             |OUTPUT   |LVDCI_33   |7             |          |NONE*    |NONE**     |         |       |LOCATED   |         |NO         |DRIVER          |
|J26       |tv_out_ycrcb<5>     |IOB      |IO_L48N_7             |OUTPUT   |LVDCI_33   |7             |          |NONE*    |NONE**     |         |       |LOCATED   |         |NO         |DRIVER          |
|J27       |tv_out_i2c_clock    |IOB      |IO_L43N_7             |OUTPUT   |LVDCI_33   |7             |          |NONE*    |NONE**     |         |       |LOCATED   |         |NO         |DRIVER          |
|J28       |systemace_data<10>  |IOB      |IO_L52N_7             |INPUT    |LVTTL      |7             |          |         |           |NONE     |       |LOCATED   |         |NO         |NONE            |
|J29       |systemace_data<11>  |IOB      |IO_L46P_7             |INPUT    |LVTTL      |7             |          |         |           |NONE     |       |LOCATED   |         |NO         |NONE            |
|J30       |systemace_address<3>|IOB      |IO_L44P_7             |OUTPUT   |LVTTL      |7             |12        |SLOW     |NONE**     |         |       |LOCATED   |         |NO         |NONE            |
|J31       |systemace_address<2>|IOB      |IO_L47P_7             |OUTPUT   |LVTTL      |7             |12        |SLOW     |NONE**     |         |       |LOCATED   |         |NO         |NONE            |
|K1        |daughtercard<33>    |IOB      |IO_L70N_2             |INPUT    |LVTTL      |2             |          |         |           |NONE     |       |LOCATED   |         |NO         |NONE            |
|K2        |daughtercard<39>    |IOB      |IO_L67N_2             |INPUT    |LVTTL      |2             |          |         |           |NONE     |       |LOCATED   |         |NO         |NONE            |
|K3        |daughtercard<31>    |IOB      |IO_L52N_2             |INPUT    |LVTTL      |2             |          |         |           |NONE     |       |LOCATED   |         |NO         |NONE            |
|K4        |                    |         |GND                   |         |           |              |          |         |           |         |       |          |         |           |                |
|K5        |daughtercard<4>     |IOB      |IO_L48P_2             |INPUT    |LVTTL      |2             |          |         |           |NONE     |       |LOCATED   |         |NO         |NONE            |
|K6        |                    |         |VCCO_2                |         |           |2             |          |         |           |         |3.30   |          |         |           |                |
|K7        |daughtercard<27>    |IOB      |IO_L27P_2/VREF_2      |INPUT    |LVTTL      |2             |          |         |           |NONE     |       |LOCATED   |         |NO         |NONE            |
|K8        |daughtercard<28>    |IOB      |IO_L25N_2             |INPUT    |LVTTL      |2             |          |         |           |NONE     |       |LOCATED   |         |NO         |NONE            |
|K9        |daughtercard<30>    |IOB      |IO_L04P_2             |INPUT    |LVTTL      |2             |          |         |           |NONE     |       |LOCATED   |         |NO         |NONE            |
|K10       |analyzer2_data<14>  |IOB      |IO_L04N_2             |OUTPUT   |LVTTL      |2             |12        |SLOW     |NONE**     |         |       |LOCATED   |         |NO         |NONE            |
|K11       |                    |         |TCK                   |         |           |              |          |         |           |         |       |          |         |           |                |
|K12       |                    |DIFFM    |IO_L51P_1             |UNUSED   |           |1             |          |         |           |         |       |          |         |           |                |
|K13       |                    |DIFFS    |IO_L51N_1/VREF_1      |UNUSED   |           |1             |          |         |           |         |       |          |         |           |                |
|K14       |                    |DIFFM    |IO_L77P_1             |UNUSED   |           |1             |          |         |           |         |       |          |         |           |                |
|K15       |                    |         |VCCINT                |         |           |              |          |         |           |         |1.5    |          |         |           |                |
|K16       |                    |         |GND                   |         |           |              |          |         |           |         |       |          |         |           |                |
|K17       |                    |         |VCCINT                |         |           |              |          |         |           |         |1.5    |          |         |           |                |
|K18       |                    |DIFFS    |IO_L91N_0/VREF_0      |UNUSED   |           |0             |          |         |           |         |       |          |         |           |                |
|K19       |                    |DIFFM    |IO_L22P_0             |UNUSED   |           |0             |          |         |           |         |       |          |         |           |                |
|K20       |                    |DIFFS    |IO_L22N_0             |UNUSED   |           |0             |          |         |           |         |       |          |         |           |                |
|K21       |                    |DIFFS    |IO_L05N_7             |UNUSED   |           |7             |          |         |           |         |       |          |         |           |                |
|K22       |analyzer3_data<13>  |IOB      |IO_L05P_7             |OUTPUT   |LVTTL      |7             |12        |SLOW     |NONE**     |         |       |LOCATED   |         |NO         |NONE            |
|K23       |analyzer3_data<5>   |IOB      |IO_L27N_7             |OUTPUT   |LVTTL      |7             |12        |SLOW     |NONE**     |         |       |LOCATED   |         |NO         |NONE            |
|K24       |analyzer3_data<15>  |IOB      |IO_L20P_7             |OUTPUT   |LVTTL      |7             |12        |SLOW     |NONE**     |         |       |LOCATED   |         |NO         |NONE            |
|K25       |analyzer3_data<14>  |IOB      |IO_L23P_7             |OUTPUT   |LVTTL      |7             |12        |SLOW     |NONE**     |         |       |LOCATED   |         |NO         |NONE            |
|K26       |                    |         |VCCO_7                |         |           |7             |          |         |           |         |3.30   |          |         |           |                |
|K27       |tv_out_subcar_reset |IOB      |IO_L43P_7             |OUTPUT   |LVDCI_33   |7             |          |NONE*    |NONE**     |         |       |LOCATED   |         |NO         |DRIVER          |
|K28       |                    |         |GND                   |         |           |              |          |         |           |         |       |          |         |           |                |
|K29       |systemace_data<9>   |IOB      |IO_L50N_7             |INPUT    |LVTTL      |7             |          |         |           |NONE     |       |LOCATED   |         |NO         |NONE            |
|K30       |systemace_address<1>|IOB      |IO_L53N_7             |OUTPUT   |LVTTL      |7             |12        |SLOW     |NONE**     |         |       |LOCATED   |         |NO         |NONE            |
|K31       |systemace_address<0>|IOB      |IO_L68N_7             |OUTPUT   |LVTTL      |7             |12        |SLOW     |NONE**     |         |       |LOCATED   |         |NO         |NONE            |
|L1        |analyzer1_data<10>  |IOB      |IO_L70P_2             |OUTPUT   |LVTTL      |2             |12        |SLOW     |NONE**     |         |       |LOCATED   |         |NO         |NONE            |
|L2        |analyzer1_data<9>   |IOB      |IO_L67P_2             |OUTPUT   |LVTTL      |2             |12        |SLOW     |NONE**     |         |       |LOCATED   |         |NO         |NONE            |
|L3        |daughtercard<34>    |IOB      |IO_L52P_2             |INPUT    |LVTTL      |2             |          |         |           |NONE     |       |LOCATED   |         |NO         |NONE            |
|L4        |daughtercard<32>    |IOB      |IO_L69N_2             |INPUT    |LVTTL      |2             |          |         |           |NONE     |       |LOCATED   |         |NO         |NONE            |
|L5        |analyzer1_data<11>  |IOB      |IO_L54N_2             |OUTPUT   |LVTTL      |2             |12        |SLOW     |NONE**     |         |       |LOCATED   |         |NO         |NONE            |
|L6        |daughtercard<25>    |IOB      |IO_L47P_2             |INPUT    |LVTTL      |2             |          |         |           |NONE     |       |LOCATED   |         |NO         |NONE            |
|L7        |daughtercard<43>    |IOB      |IO_L51N_2             |INPUT    |LVTTL      |2             |          |         |           |NONE     |       |LOCATED   |         |NO         |NONE            |
|L8        |daughtercard<26>    |IOB      |IO_L25P_2             |INPUT    |LVTTL      |2             |          |         |           |NONE     |       |LOCATED   |         |NO         |NONE            |
|L9        |daughtercard<29>    |IOB      |IO_L44N_2             |INPUT    |LVTTL      |2             |          |         |           |NONE     |       |LOCATED   |         |NO         |NONE            |
|L10       |analyzer2_data<13>  |IOB      |IO_L19N_2             |OUTPUT   |LVTTL      |2             |12        |SLOW     |NONE**     |         |       |LOCATED   |         |NO         |NONE            |
|L11       |                    |         |VCCINT                |         |           |              |          |         |           |         |1.5    |          |         |           |                |
|L12       |                    |         |VCCO_1                |         |           |1             |          |         |           |         |3.30   |          |         |           |                |
|L13       |                    |         |VCCO_1                |         |           |1             |          |         |           |         |3.30   |          |         |           |                |
|L14       |                    |         |VCCO_1                |         |           |1             |          |         |           |         |3.30   |          |         |           |                |
|L15       |                    |         |VCCO_1                |         |           |1             |          |         |           |         |3.30   |          |         |           |                |
|L16       |                    |         |VCCINT                |         |           |              |          |         |           |         |1.5    |          |         |           |                |
|L17       |                    |         |VCCO_0                |         |           |0             |          |         |           |         |3.30   |          |         |           |                |
|L18       |                    |         |VCCO_0                |         |           |0             |          |         |           |         |3.30   |          |         |           |                |
|L19       |                    |         |VCCO_0                |         |           |0             |          |         |           |         |3.30   |          |         |           |                |
|L20       |                    |         |VCCO_0                |         |           |0             |          |         |           |         |3.30   |          |         |           |                |
|L21       |                    |         |VCCINT                |         |           |              |          |         |           |         |1.5    |          |         |           |                |
|L22       |analyzer3_data<10>  |IOB      |IO_L45N_7             |OUTPUT   |LVTTL      |7             |12        |SLOW     |NONE**     |         |       |LOCATED   |         |NO         |NONE            |
|L23       |analyzer3_data<9>   |IOB      |IO_L27P_7/VREF_7      |OUTPUT   |LVTTL      |7             |12        |SLOW     |NONE**     |         |       |LOCATED   |         |NO         |NONE            |
|L24       |analyzer3_data<12>  |IOB      |IO_L51N_7             |OUTPUT   |LVTTL      |7             |12        |SLOW     |NONE**     |         |       |LOCATED   |         |NO         |NONE            |
|L25       |analyzer3_data<11>  |IOB      |IO_L49N_7             |OUTPUT   |LVTTL      |7             |12        |SLOW     |NONE**     |         |       |LOCATED   |         |NO         |NONE            |
|L26       |tv_out_ycrcb<4>     |IOB      |IO_L48P_7             |OUTPUT   |LVDCI_33   |7             |          |NONE*    |NONE**     |         |       |LOCATED   |         |NO         |DRIVER          |
|L27       |tv_out_clock        |IOB      |IO_L67N_7             |OUTPUT   |LVDCI_33   |7             |          |NONE*    |NONE**     |         |       |LOCATED   |         |NO         |DRIVER          |
|L28       |systemace_data<7>   |IOB      |IO_L52P_7             |INPUT    |LVTTL      |7             |          |         |           |NONE     |       |LOCATED   |         |NO         |NONE            |
|L29       |systemace_data<8>   |IOB      |IO_L50P_7             |INPUT    |LVTTL      |7             |          |         |           |NONE     |       |LOCATED   |         |NO         |NONE            |
|L30       |tv_in_ycrcb<2>      |IOB      |IO_L53P_7             |INPUT    |LVTTL      |7             |          |         |           |NONE     |       |LOCATED   |         |NO         |NONE            |
|L31       |systemace_mpbrdy    |IOB      |IO_L68P_7             |INPUT    |LVTTL      |7             |          |         |           |NONE     |       |LOCATED   |         |NO         |NONE            |
|M1        |analyzer1_data<7>   |IOB      |IO_L76N_2             |OUTPUT   |LVTTL      |2             |12        |SLOW     |NONE**     |         |       |LOCATED   |         |NO         |NONE            |
|M2        |analyzer1_data<6>   |IOB      |IO_L75N_2             |OUTPUT   |LVTTL      |2             |12        |SLOW     |NONE**     |         |       |LOCATED   |         |NO         |NONE            |
|M3        |daughtercard<36>    |IOB      |IO_L73N_2             |INPUT    |LVTTL      |2             |          |         |           |NONE     |       |LOCATED   |         |NO         |NONE            |
|M4        |daughtercard<35>    |IOB      |IO_L69P_2/VREF_2      |INPUT    |LVTTL      |2             |          |         |           |NONE     |       |LOCATED   |         |NO         |NONE            |
|M5        |daughtercard<24>    |IOB      |IO_L54P_2             |INPUT    |LVTTL      |2             |          |         |           |NONE     |       |LOCATED   |         |NO         |NONE            |
|M6        |daughtercard<37>    |IOB      |IO_L68N_2             |INPUT    |LVTTL      |2             |          |         |           |NONE     |       |LOCATED   |         |NO         |NONE            |
|M7        |daughtercard<38>    |IOB      |IO_L51P_2/VREF_2      |INPUT    |LVTTL      |2             |          |         |           |NONE     |       |LOCATED   |         |NO         |NONE            |
|M8        |analyzer1_data<12>  |IOB      |IO_L53N_2             |OUTPUT   |LVTTL      |2             |12        |SLOW     |NONE**     |         |       |LOCATED   |         |NO         |NONE            |
|M9        |analyzer1_data<13>  |IOB      |IO_L44P_2             |OUTPUT   |LVTTL      |2             |12        |SLOW     |NONE**     |         |       |LOCATED   |         |NO         |NONE            |
|M10       |analyzer2_data<12>  |IOB      |IO_L19P_2             |OUTPUT   |LVTTL      |2             |12        |SLOW     |NONE**     |         |       |LOCATED   |         |NO         |NONE            |
|M11       |                    |         |VCCO_2                |         |           |2             |          |         |           |         |3.30   |          |         |           |                |
|M12       |                    |         |VCCINT                |         |           |              |          |         |           |         |1.5    |          |         |           |                |
|M13       |                    |         |VCCO_1                |         |           |1             |          |         |           |         |3.30   |          |         |           |                |
|M14       |                    |         |VCCO_1                |         |           |1             |          |         |           |         |3.30   |          |         |           |                |
|M15       |                    |         |VCCO_1                |         |           |1             |          |         |           |         |3.30   |          |         |           |                |
|M16       |                    |         |VCCINT                |         |           |              |          |         |           |         |1.5    |          |         |           |                |
|M17       |                    |         |VCCO_0                |         |           |0             |          |         |           |         |3.30   |          |         |           |                |
|M18       |                    |         |VCCO_0                |         |           |0             |          |         |           |         |3.30   |          |         |           |                |
|M19       |                    |         |VCCO_0                |         |           |0             |          |         |           |         |3.30   |          |         |           |                |
|M20       |                    |         |VCCINT                |         |           |              |          |         |           |         |1.5    |          |         |           |                |
|M21       |                    |         |VCCO_7                |         |           |7             |          |         |           |         |3.30   |          |         |           |                |
|M22       |analyzer3_data<4>   |IOB      |IO_L45P_7/VREF_7      |OUTPUT   |LVTTL      |7             |12        |SLOW     |NONE**     |         |       |LOCATED   |         |NO         |NONE            |
|M23       |analyzer3_data<8>   |IOB      |IO_L54N_7             |OUTPUT   |LVTTL      |7             |12        |SLOW     |NONE**     |         |       |LOCATED   |         |NO         |NONE            |
|M24       |analyzer3_data<7>   |IOB      |IO_L51P_7/VREF_7      |OUTPUT   |LVTTL      |7             |12        |SLOW     |NONE**     |         |       |LOCATED   |         |NO         |NONE            |
|M25       |analyzer3_data<6>   |IOB      |IO_L49P_7             |OUTPUT   |LVTTL      |7             |12        |SLOW     |NONE**     |         |       |LOCATED   |         |NO         |NONE            |
|M26       |tv_out_ycrcb<3>     |IOB      |IO_L69N_7             |OUTPUT   |LVDCI_33   |7             |          |NONE*    |NONE**     |         |       |LOCATED   |         |NO         |DRIVER          |
|M27       |tv_out_vsync_b      |IOB      |IO_L67P_7             |OUTPUT   |LVDCI_33   |7             |          |NONE*    |NONE**     |         |       |LOCATED   |         |NO         |DRIVER          |
|M28       |systemace_data<5>   |IOB      |IO_L70N_7             |INPUT    |LVTTL      |7             |          |         |           |NONE     |       |LOCATED   |         |NO         |NONE            |
|M29       |systemace_data<6>   |IOB      |IO_L71N_7             |INPUT    |LVTTL      |7             |          |         |           |NONE     |       |LOCATED   |         |NO         |NONE            |
|M30       |tv_in_ycrcb<0>      |IOB      |IO_L74N_7             |INPUT    |LVTTL      |7             |          |         |           |NONE     |       |LOCATED   |         |NO         |NONE            |
|M31       |tv_in_ycrcb<1>      |IOB      |IO_L76N_7             |INPUT    |LVTTL      |7             |          |         |           |NONE     |       |LOCATED   |         |NO         |NONE            |
|N1        |analyzer1_data<5>   |IOB      |IO_L76P_2             |OUTPUT   |LVTTL      |2             |12        |SLOW     |NONE**     |         |       |LOCATED   |         |NO         |NONE            |
|N2        |analyzer1_data<4>   |IOB      |IO_L75P_2/VREF_2      |OUTPUT   |LVTTL      |2             |12        |SLOW     |NONE**     |         |       |LOCATED   |         |NO         |NONE            |
|N3        |analyzer2_data<10>  |IOB      |IO_L73P_2             |OUTPUT   |LVTTL      |2             |12        |SLOW     |NONE**     |         |       |LOCATED   |         |NO         |NONE            |
|N4        |analyzer2_data<4>   |IOB      |IO_L78N_2             |OUTPUT   |LVTTL      |2             |12        |SLOW     |NONE**     |         |       |LOCATED   |         |NO         |NONE            |
|N5        |daughtercard<23>    |IOB      |IO_L72N_2             |INPUT    |LVTTL      |2             |          |         |           |NONE     |       |LOCATED   |         |NO         |NONE            |
|N6        |analyzer2_data<6>   |IOB      |IO_L68P_2             |OUTPUT   |LVTTL      |2             |12        |SLOW     |NONE**     |         |       |LOCATED   |         |NO         |NONE            |
|N7        |                    |         |GND                   |         |           |              |          |         |           |         |       |          |         |           |                |
|N8        |rs232_cts           |IOB      |IO_L53P_2             |INPUT    |LVTTL      |2             |          |         |           |NONE     |       |LOCATED   |         |NO         |NONE            |
|N9        |analyzer1_data<8>   |IOB      |IO_L71N_2             |OUTPUT   |LVTTL      |2             |12        |SLOW     |NONE**     |         |       |LOCATED   |         |NO         |NONE            |
|N10       |                    |DIFFS    |IO_L50N_2             |UNUSED   |           |2             |          |         |           |         |       |          |         |           |                |
|N11       |                    |         |VCCO_2                |         |           |2             |          |         |           |         |3.30   |          |         |           |                |
|N12       |                    |         |VCCO_2                |         |           |2             |          |         |           |         |3.30   |          |         |           |                |
|N13       |                    |         |VCCINT                |         |           |              |          |         |           |         |1.5    |          |         |           |                |
|N14       |                    |         |VCCINT                |         |           |              |          |         |           |         |1.5    |          |         |           |                |
|N15       |                    |         |VCCINT                |         |           |              |          |         |           |         |1.5    |          |         |           |                |
|N16       |                    |         |VCCINT                |         |           |              |          |         |           |         |1.5    |          |         |           |                |
|N17       |                    |         |VCCINT                |         |           |              |          |         |           |         |1.5    |          |         |           |                |
|N18       |                    |         |VCCINT                |         |           |              |          |         |           |         |1.5    |          |         |           |                |
|N19       |                    |         |VCCINT                |         |           |              |          |         |           |         |1.5    |          |         |           |                |
|N20       |                    |         |VCCO_7                |         |           |7             |          |         |           |         |3.30   |          |         |           |                |
|N21       |                    |         |VCCO_7                |         |           |7             |          |         |           |         |3.30   |          |         |           |                |
|N22       |                    |DIFFS    |IO_L72N_7             |UNUSED   |           |7             |          |         |           |         |       |          |         |           |                |
|N23       |analyzer3_data<3>   |IOB      |IO_L54P_7             |OUTPUT   |LVTTL      |7             |12        |SLOW     |NONE**     |         |       |LOCATED   |         |NO         |NONE            |
|N24       |                    |DIFFS    |IO_L95N_7             |UNUSED   |           |7             |          |         |           |         |       |          |         |           |                |
|N25       |                    |         |GND                   |         |           |              |          |         |           |         |       |          |         |           |                |
|N26       |tv_out_ycrcb<2>     |IOB      |IO_L69P_7/VREF_7      |OUTPUT   |LVDCI_33   |7             |          |NONE*    |NONE**     |         |       |LOCATED   |         |NO         |DRIVER          |
|N27       |tv_out_hsync_b      |IOB      |IO_L73N_7             |OUTPUT   |LVDCI_33   |7             |          |NONE*    |NONE**     |         |       |LOCATED   |         |NO         |DRIVER          |
|N28       |systemace_data<3>   |IOB      |IO_L70P_7             |INPUT    |LVTTL      |7             |          |         |           |NONE     |       |LOCATED   |         |NO         |NONE            |
|N29       |systemace_data<4>   |IOB      |IO_L71P_7             |INPUT    |LVTTL      |7             |          |         |           |NONE     |       |LOCATED   |         |NO         |NONE            |
|N30       |                    |DIFFM    |IO_L74P_7             |UNUSED   |           |7             |          |         |           |         |       |          |         |           |                |
|N31       |                    |DIFFM    |IO_L76P_7             |UNUSED   |           |7             |          |         |           |         |       |          |         |           |                |
|P1        |analyzer1_data<3>   |IOB      |IO_L95N_2             |OUTPUT   |LVTTL      |2             |12        |SLOW     |NONE**     |         |       |LOCATED   |         |NO         |NONE            |
|P2        |analyzer1_data<2>   |IOB      |IO_L93N_2             |OUTPUT   |LVTTL      |2             |12        |SLOW     |NONE**     |         |       |LOCATED   |         |NO         |NONE            |
|P3        |                    |         |VCCO_2                |         |           |2             |          |         |           |         |3.30   |          |         |           |                |
|P4        |rs232_txd           |IOB      |IO_L78P_2             |OUTPUT   |LVDCI_33   |2             |          |NONE*    |NONE**     |         |       |LOCATED   |         |NO         |DRIVER          |
|P5        |daughtercard<22>    |IOB      |IO_L72P_2             |INPUT    |LVTTL      |2             |          |         |           |NONE     |       |LOCATED   |         |NO         |NONE            |
|P6        |rs232_rxd           |IOB      |IO_L92N_2             |INPUT    |LVTTL      |2             |          |         |           |NONE     |       |LOCATED   |         |NO         |NONE            |
|P7        |analyzer2_data<5>   |IOB      |IO_L77N_2             |OUTPUT   |LVTTL      |2             |12        |SLOW     |NONE**     |         |       |LOCATED   |         |NO         |NONE            |
|P8        |                    |         |VCCO_2                |         |           |2             |          |         |           |         |3.30   |          |         |           |                |
|P9        |analyzer2_data<7>   |IOB      |IO_L71P_2             |OUTPUT   |LVTTL      |2             |12        |SLOW     |NONE**     |         |       |LOCATED   |         |NO         |NONE            |
|P10       |                    |DIFFM    |IO_L50P_2             |UNUSED   |           |2             |          |         |           |         |       |          |         |           |                |
|P11       |                    |         |VCCO_2                |         |           |2             |          |         |           |         |3.30   |          |         |           |                |
|P12       |                    |         |VCCO_2                |         |           |2             |          |         |           |         |3.30   |          |         |           |                |
|P13       |                    |         |VCCINT                |         |           |              |          |         |           |         |1.5    |          |         |           |                |
|P14       |                    |         |GND                   |         |           |              |          |         |           |         |       |          |         |           |                |
|P15       |                    |         |GND                   |         |           |              |          |         |           |         |       |          |         |           |                |
|P16       |                    |         |GND                   |         |           |              |          |         |           |         |       |          |         |           |                |
|P17       |                    |         |GND                   |         |           |              |          |         |           |         |       |          |         |           |                |
|P18       |                    |         |GND                   |         |           |              |          |         |           |         |       |          |         |           |                |
|P19       |                    |         |VCCINT                |         |           |              |          |         |           |         |1.5    |          |         |           |                |
|P20       |                    |         |VCCO_7                |         |           |7             |          |         |           |         |3.30   |          |         |           |                |
|P21       |                    |         |VCCO_7                |         |           |7             |          |         |           |         |3.30   |          |         |           |                |
|P22       |                    |DIFFM    |IO_L72P_7             |UNUSED   |           |7             |          |         |           |         |       |          |         |           |                |
|P23       |analyzer3_data<2>   |IOB      |IO_L75N_7             |OUTPUT   |LVTTL      |7             |12        |SLOW     |NONE**     |         |       |LOCATED   |         |NO         |NONE            |
|P24       |                    |         |VCCO_7                |         |           |7             |          |         |           |         |3.30   |          |         |           |                |
|P25       |                    |DIFFS    |IO_L78N_7             |UNUSED   |           |7             |          |         |           |         |       |          |         |           |                |
|P26       |tv_out_ycrcb<1>     |IOB      |IO_L92N_7             |OUTPUT   |LVDCI_33   |7             |          |NONE*    |NONE**     |         |       |LOCATED   |         |NO         |DRIVER          |
|P27       |tv_out_ycrcb<9>     |IOB      |IO_L73P_7             |OUTPUT   |LVDCI_33   |7             |          |NONE*    |NONE**     |         |       |LOCATED   |         |NO         |DRIVER          |
|P28       |systemace_data<2>   |IOB      |IO_L77N_7             |INPUT    |LVTTL      |7             |          |         |           |NONE     |       |LOCATED   |         |NO         |NONE            |
|P29       |                    |         |VCCO_7                |         |           |7             |          |         |           |         |3.30   |          |         |           |                |
|P30       |                    |DIFFS    |IO_L91N_7             |UNUSED   |           |7             |          |         |           |         |       |          |         |           |                |
|P31       |systemace_we_b      |IOB      |IO_L93N_7             |OUTPUT   |LVTTL      |7             |12        |SLOW     |NONE**     |         |       |LOCATED   |         |NO         |NONE            |
|R1        |analyzer1_data<1>   |IOB      |IO_L95P_2             |OUTPUT   |LVTTL      |2             |12        |SLOW     |NONE**     |         |       |LOCATED   |         |NO         |NONE            |
|R2        |analyzer1_data<0>   |IOB      |IO_L93P_2/VREF_2      |OUTPUT   |LVTTL      |2             |12        |SLOW     |NONE**     |         |       |LOCATED   |         |NO         |NONE            |
|R3        |rs232_rts           |IOB      |IO_L96P_2             |OUTPUT   |LVDCI_33   |2             |          |NONE*    |NONE**     |         |       |LOCATED   |         |NO         |DRIVER          |
|R4        |                    |DIFFS    |IO_L96N_2             |UNUSED   |           |2             |          |         |           |         |       |          |         |           |                |
|R5        |analyzer2_data<0>   |IOB      |IO_L94N_2             |OUTPUT   |LVTTL      |2             |12        |SLOW     |NONE**     |         |       |LOCATED   |         |NO         |NONE            |
|R6        |analyzer2_data<1>   |IOB      |IO_L92P_2             |OUTPUT   |LVTTL      |2             |12        |SLOW     |NONE**     |         |       |LOCATED   |         |NO         |NONE            |
|R7        |analyzer2_data<11>  |IOB      |IO_L77P_2             |OUTPUT   |LVTTL      |2             |12        |SLOW     |NONE**     |         |       |LOCATED   |         |NO         |NONE            |
|R8        |analyzer2_data<9>   |IOB      |IO_L74N_2             |OUTPUT   |LVTTL      |2             |12        |SLOW     |NONE**     |         |       |LOCATED   |         |NO         |NONE            |
|R9        |analyzer2_data<8>   |IOB      |IO_L74P_2             |OUTPUT   |LVTTL      |2             |12        |SLOW     |NONE**     |         |       |LOCATED   |         |NO         |NONE            |
|R10       |                    |         |VCCINT                |         |           |              |          |         |           |         |1.5    |          |         |           |                |
|R11       |                    |         |VCCO_2                |         |           |2             |          |         |           |         |3.30   |          |         |           |                |
|R12       |                    |         |VCCO_2                |         |           |2             |          |         |           |         |3.30   |          |         |           |                |
|R13       |                    |         |VCCINT                |         |           |              |          |         |           |         |1.5    |          |         |           |                |
|R14       |                    |         |GND                   |         |           |              |          |         |           |         |       |          |         |           |                |
|R15       |                    |         |GND                   |         |           |              |          |         |           |         |       |          |         |           |                |
|R16       |                    |         |GND                   |         |           |              |          |         |           |         |       |          |         |           |                |
|R17       |                    |         |GND                   |         |           |              |          |         |           |         |       |          |         |           |                |
|R18       |                    |         |GND                   |         |           |              |          |         |           |         |       |          |         |           |                |
|R19       |                    |         |VCCINT                |         |           |              |          |         |           |         |1.5    |          |         |           |                |
|R20       |                    |         |VCCO_7                |         |           |7             |          |         |           |         |3.30   |          |         |           |                |
|R21       |                    |         |VCCO_7                |         |           |7             |          |         |           |         |3.30   |          |         |           |                |
|R22       |                    |         |VCCINT                |         |           |              |          |         |           |         |1.5    |          |         |           |                |
|R23       |analyzer3_data<1>   |IOB      |IO_L75P_7/VREF_7      |OUTPUT   |LVTTL      |7             |12        |SLOW     |NONE**     |         |       |LOCATED   |         |NO         |NONE            |
|R24       |analyzer3_data<0>   |IOB      |IO_L95P_7             |OUTPUT   |LVTTL      |7             |12        |SLOW     |NONE**     |         |       |LOCATED   |         |NO         |NONE            |
|R25       |tv_in_ycrcb<3>      |IOB      |IO_L78P_7             |INPUT    |LVTTL      |7             |          |         |           |NONE     |       |LOCATED   |         |NO         |NONE            |
|R26       |tv_out_ycrcb<0>     |IOB      |IO_L92P_7             |OUTPUT   |LVDCI_33   |7             |          |NONE*    |NONE**     |         |       |LOCATED   |         |NO         |DRIVER          |
|R27       |tv_out_ycrcb<8>     |IOB      |IO_L96N_7             |OUTPUT   |LVDCI_33   |7             |          |NONE*    |NONE**     |         |       |LOCATED   |         |NO         |DRIVER          |
|R28       |systemace_data<0>   |IOB      |IO_L77P_7             |INPUT    |LVTTL      |7             |          |         |           |NONE     |       |LOCATED   |         |NO         |NONE            |
|R29       |systemace_data<1>   |IOB      |IO_L94N_7             |INPUT    |LVTTL      |7             |          |         |           |NONE     |       |LOCATED   |         |NO         |NONE            |
|R30       |                    |DIFFM    |IO_L91P_7             |UNUSED   |           |7             |          |         |           |         |       |          |         |           |                |
|R31       |systemace_oe_b      |IOB      |IO_L93P_7/VREF_7      |OUTPUT   |LVTTL      |7             |12        |SLOW     |NONE**     |         |       |LOCATED   |         |NO         |NONE            |
|T1        |                    |         |GND                   |         |           |              |          |         |           |         |       |          |         |           |                |
|T2        |                    |         |VCCAUX                |         |           |              |          |         |           |         |3.3    |          |         |           |                |
|T3        |                    |DIFFS    |IO_L94N_3             |UNUSED   |           |3             |          |         |           |         |       |          |         |           |                |
|T4        |                    |         |GND                   |         |           |              |          |         |           |         |       |          |         |           |                |
|T5        |                    |DIFFM    |IO_L94P_2             |UNUSED   |           |2             |          |         |           |         |       |          |         |           |                |
|T6        |                    |DIFFS    |IO_L96N_3             |UNUSED   |           |3             |          |         |           |         |       |          |         |           |                |
|T7        |                    |         |GND                   |         |           |              |          |         |           |         |       |          |         |           |                |
|T8        |analyzer2_data<3>   |IOB      |IO_L91N_2             |OUTPUT   |LVTTL      |2             |12        |SLOW     |NONE**     |         |       |LOCATED   |         |NO         |NONE            |
|T9        |analyzer2_data<2>   |IOB      |IO_L91P_2             |OUTPUT   |LVTTL      |2             |12        |SLOW     |NONE**     |         |       |LOCATED   |         |NO         |NONE            |
|T10       |                    |         |GND                   |         |           |              |          |         |           |         |       |          |         |           |                |
|T11       |                    |         |VCCINT                |         |           |              |          |         |           |         |1.5    |          |         |           |                |
|T12       |                    |         |VCCINT                |         |           |              |          |         |           |         |1.5    |          |         |           |                |
|T13       |                    |         |VCCINT                |         |           |              |          |         |           |         |1.5    |          |         |           |                |
|T14       |                    |         |GND                   |         |           |              |          |         |           |         |       |          |         |           |                |
|T15       |                    |         |GND                   |         |           |              |          |         |           |         |       |          |         |           |                |
|T16       |                    |         |GND                   |         |           |              |          |         |           |         |       |          |         |           |                |
|T17       |                    |         |GND                   |         |           |              |          |         |           |         |       |          |         |           |                |
|T18       |                    |         |GND                   |         |           |              |          |         |           |         |       |          |         |           |                |
|T19       |                    |         |VCCINT                |         |           |              |          |         |           |         |1.5    |          |         |           |                |
|T20       |                    |         |VCCINT                |         |           |              |          |         |           |         |1.5    |          |         |           |                |
|T21       |                    |         |VCCINT                |         |           |              |          |         |           |         |1.5    |          |         |           |                |
|T22       |                    |         |GND                   |         |           |              |          |         |           |         |       |          |         |           |                |
|T23       |tv_in_ycrcb<6>      |IOB      |IO_L91N_6             |INPUT    |LVTTL      |6             |          |         |           |NONE     |       |LOCATED   |         |NO         |NONE            |
|T24       |tv_in_ycrcb<4>      |IOB      |IO_L94N_6             |INPUT    |LVTTL      |6             |          |         |           |NONE     |       |LOCATED   |         |NO         |NONE            |
|T25       |                    |         |GND                   |         |           |              |          |         |           |         |       |          |         |           |                |
|T26       |tv_in_ycrcb<5>      |IOB      |IO_L92N_6             |INPUT    |LVTTL      |6             |          |         |           |NONE     |       |LOCATED   |         |NO         |NONE            |
|T27       |                    |DIFFM    |IO_L96P_7             |UNUSED   |           |7             |          |         |           |         |       |          |         |           |                |
|T28       |                    |         |GND                   |         |           |              |          |         |           |         |       |          |         |           |                |
|T29       |tv_out_ycrcb<7>     |IOB      |IO_L94P_7             |OUTPUT   |LVDCI_33   |7             |          |NONE*    |NONE**     |         |       |LOCATED   |         |NO         |DRIVER          |
|T30       |                    |         |VCCAUX                |         |           |              |          |         |           |         |3.3    |          |         |           |                |
|T31       |                    |         |GND                   |         |           |              |          |         |           |         |       |          |         |           |                |
|U1        |ram1_bwe_b<1>       |IOB      |IO_L93N_3/VREF_3      |OUTPUT   |LVDCI_33   |3             |          |NONE*    |NONE**     |         |       |LOCATED   |         |NO         |DRIVER          |
|U2        |ram1_bwe_b<0>       |IOB      |IO_L91N_3             |OUTPUT   |LVDCI_33   |3             |          |NONE*    |NONE**     |         |       |LOCATED   |         |NO         |DRIVER          |
|U3        |ram1_address<7>     |IOB      |IO_L94P_3             |OUTPUT   |LVDCI_33   |3             |          |NONE*    |NONE**     |         |       |LOCATED   |         |NO         |DRIVER          |
|U4        |ram1_ce_b           |IOB      |IO_L77N_3             |OUTPUT   |LVDCI_33   |3             |          |NONE*    |NONE**     |         |       |LOCATED   |         |NO         |DRIVER          |
|U5        |ram1_bwe_b<3>       |IOB      |IO_L96P_3             |OUTPUT   |LVDCI_33   |3             |          |NONE*    |NONE**     |         |       |LOCATED   |         |NO         |DRIVER          |
|U6        |ram1_address<16>    |IOB      |IO_L95N_3             |OUTPUT   |LVDCI_33   |3             |          |NONE*    |NONE**     |         |       |LOCATED   |         |NO         |DRIVER          |
|U7        |analyzer4_data<1>   |IOB      |IO_L78N_3             |OUTPUT   |LVTTL      |3             |12        |SLOW     |NONE**     |         |       |LOCATED   |         |NO         |NONE            |
|U8        |analyzer4_data<0>   |IOB      |IO_L92N_3             |OUTPUT   |LVTTL      |3             |12        |SLOW     |NONE**     |         |       |LOCATED   |         |NO         |NONE            |
|U9        |                    |DIFFS    |IO_L69N_3/VREF_3      |UNUSED   |           |3             |          |         |           |         |       |          |         |           |                |
|U10       |                    |         |VCCINT                |         |           |              |          |         |           |         |1.5    |          |         |           |                |
|U11       |                    |         |VCCO_3                |         |           |3             |          |         |           |         |3.30   |          |         |           |                |
|U12       |                    |         |VCCO_3                |         |           |3             |          |         |           |         |3.30   |          |         |           |                |
|U13       |                    |         |VCCINT                |         |           |              |          |         |           |         |1.5    |          |         |           |                |
|U14       |                    |         |GND                   |         |           |              |          |         |           |         |       |          |         |           |                |
|U15       |                    |         |GND                   |         |           |              |          |         |           |         |       |          |         |           |                |
|U16       |                    |         |GND                   |         |           |              |          |         |           |         |       |          |         |           |                |
|U17       |                    |         |GND                   |         |           |              |          |         |           |         |       |          |         |           |                |
|U18       |                    |         |GND                   |         |           |              |          |         |           |         |       |          |         |           |                |
|U19       |                    |         |VCCINT                |         |           |              |          |         |           |         |1.5    |          |         |           |                |
|U20       |                    |         |VCCO_6                |         |           |6             |          |         |           |         |3.30   |          |         |           |                |
|U21       |                    |         |VCCO_6                |         |           |6             |          |         |           |         |3.30   |          |         |           |                |
|U22       |                    |         |VCCINT                |         |           |              |          |         |           |         |1.5    |          |         |           |                |
|U23       |tv_in_ycrcb<7>      |IOB      |IO_L91P_6             |INPUT    |LVTTL      |6             |          |         |           |NONE     |       |LOCATED   |         |NO         |NONE            |
|U24       |                    |DIFFM    |IO_L94P_6             |UNUSED   |           |6             |          |         |           |         |       |          |         |           |                |
|U25       |ram0_cen_b          |IOB      |IO_L72N_6             |OUTPUT   |LVDCI_33   |6             |          |NONE*    |NONE**     |         |       |LOCATED   |         |NO         |DRIVER          |
|U26       |ram0_bwe_b<3>       |IOB      |IO_L92P_6             |OUTPUT   |LVDCI_33   |6             |          |NONE*    |NONE**     |         |       |LOCATED   |         |NO         |DRIVER          |
|U27       |ram0_bwe_b<1>       |IOB      |IO_L77N_6             |OUTPUT   |LVDCI_33   |6             |          |NONE*    |NONE**     |         |       |LOCATED   |         |NO         |DRIVER          |
|U28       |ram0_data<9>        |IOB      |IO_L93N_6/VREF_6      |INPUT    |LVDCI_33   |6             |          |         |           |NONE     |       |LOCATED   |         |NO         |NONE            |
|U29       |ram0_data<10>       |IOB      |IO_L78N_6             |INPUT    |LVDCI_33   |6             |          |         |           |NONE     |       |LOCATED   |         |NO         |NONE            |
|U30       |ram0_clk            |IOB      |IO_L95N_6             |OUTPUT   |LVDCI_33   |6             |          |NONE*    |NONE**     |         |       |LOCATED   |         |NO         |DRIVER          |
|U31       |ram0_we_b           |IOB      |IO_L96N_6             |OUTPUT   |LVDCI_33   |6             |          |NONE*    |NONE**     |         |       |LOCATED   |         |NO         |DRIVER          |
|V1        |ram1_bwe_b<2>       |IOB      |IO_L93P_3             |OUTPUT   |LVDCI_33   |3             |          |NONE*    |NONE**     |         |       |LOCATED   |         |NO         |DRIVER          |
|V2        |ram1_data<17>       |IOB      |IO_L91P_3             |INPUT    |LVDCI_33   |3             |          |         |           |NONE     |       |LOCATED   |         |NO         |NONE            |
|V3        |                    |         |VCCO_3                |         |           |3             |          |         |           |         |3.30   |          |         |           |                |
|V4        |ram1_data<8>        |IOB      |IO_L77P_3             |INPUT    |LVDCI_33   |3             |          |         |           |NONE     |       |LOCATED   |         |NO         |NONE            |
|V5        |ram1_cen_b          |IOB      |IO_L75N_3/VREF_3      |OUTPUT   |LVDCI_33   |3             |          |NONE*    |NONE**     |         |       |LOCATED   |         |NO         |DRIVER          |
|V6        |ram1_address<15>    |IOB      |IO_L95P_3             |OUTPUT   |LVDCI_33   |3             |          |NONE*    |NONE**     |         |       |LOCATED   |         |NO         |DRIVER          |
|V7        |analyzer4_data<2>   |IOB      |IO_L78P_3             |OUTPUT   |LVTTL      |3             |12        |SLOW     |NONE**     |         |       |LOCATED   |         |NO         |NONE            |
|V8        |                    |         |VCCO_3                |         |           |3             |          |         |           |         |3.30   |          |         |           |                |
|V9        |                    |DIFFM    |IO_L69P_3             |UNUSED   |           |3             |          |         |           |         |       |          |         |           |                |
|V10       |                    |DIFFS    |IO_L51N_3/VREF_3      |UNUSED   |           |3             |          |         |           |         |       |          |         |           |                |
|V11       |                    |         |VCCO_3                |         |           |3             |          |         |           |         |3.30   |          |         |           |                |
|V12       |                    |         |VCCO_3                |         |           |3             |          |         |           |         |3.30   |          |         |           |                |
|V13       |                    |         |VCCINT                |         |           |              |          |         |           |         |1.5    |          |         |           |                |
|V14       |                    |         |GND                   |         |           |              |          |         |           |         |       |          |         |           |                |
|V15       |                    |         |GND                   |         |           |              |          |         |           |         |       |          |         |           |                |
|V16       |                    |         |GND                   |         |           |              |          |         |           |         |       |          |         |           |                |
|V17       |                    |         |GND                   |         |           |              |          |         |           |         |       |          |         |           |                |
|V18       |                    |         |GND                   |         |           |              |          |         |           |         |       |          |         |           |                |
|V19       |                    |         |VCCINT                |         |           |              |          |         |           |         |1.5    |          |         |           |                |
|V20       |                    |         |VCCO_6                |         |           |6             |          |         |           |         |3.30   |          |         |           |                |
|V21       |                    |         |VCCO_6                |         |           |6             |          |         |           |         |3.30   |          |         |           |                |
|V22       |                    |DIFFS    |IO_L53N_6             |UNUSED   |           |6             |          |         |           |         |       |          |         |           |                |
|V23       |tv_in_ycrcb<8>      |IOB      |IO_L74N_6             |INPUT    |LVTTL      |6             |          |         |           |NONE     |       |LOCATED   |         |NO         |NONE            |
|V24       |                    |         |VCCO_6                |         |           |6             |          |         |           |         |3.30   |          |         |           |                |
|V25       |ram0_oe_b           |IOB      |IO_L72P_6             |OUTPUT   |LVDCI_33   |6             |          |NONE*    |NONE**     |         |       |LOCATED   |         |NO         |DRIVER          |
|V26       |ram0_adv_ld         |IOB      |IO_L68N_6             |OUTPUT   |LVDCI_33   |6             |          |NONE*    |NONE**     |         |       |LOCATED   |         |NO         |DRIVER          |
|V27       |ram0_bwe_b<0>       |IOB      |IO_L77P_6             |OUTPUT   |LVDCI_33   |6             |          |NONE*    |NONE**     |         |       |LOCATED   |         |NO         |DRIVER          |
|V28       |ram0_data<11>       |IOB      |IO_L93P_6             |INPUT    |LVDCI_33   |6             |          |         |           |NONE     |       |LOCATED   |         |NO         |NONE            |
|V29       |                    |         |VCCO_6                |         |           |6             |          |         |           |         |3.30   |          |         |           |                |
|V30       |                    |DIFFM    |IO_L95P_6             |UNUSED   |           |6             |          |         |           |         |       |          |         |           |                |
|V31       |ram0_address<18>    |IOB      |IO_L96P_6             |OUTPUT   |LVDCI_33   |6             |          |NONE*    |NONE**     |         |       |LOCATED   |         |NO         |DRIVER          |
|W1        |                    |DIFFS    |IO_L76N_3             |UNUSED   |           |3             |          |         |           |         |       |          |         |           |                |
|W2        |                    |DIFFS    |IO_L74N_3             |UNUSED   |           |3             |          |         |           |         |       |          |         |           |                |
|W3        |ram1_data<0>        |IOB      |IO_L71N_3             |INPUT    |LVDCI_33   |3             |          |         |           |NONE     |       |LOCATED   |         |NO         |NONE            |
|W4        |ram1_address<6>     |IOB      |IO_L70N_3             |OUTPUT   |LVDCI_33   |3             |          |NONE*    |NONE**     |         |       |LOCATED   |         |NO         |DRIVER          |
|W5        |ram1_oe_b           |IOB      |IO_L75P_3             |OUTPUT   |LVDCI_33   |3             |          |NONE*    |NONE**     |         |       |LOCATED   |         |NO         |DRIVER          |
|W6        |ram1_address<14>    |IOB      |IO_L73N_3             |OUTPUT   |LVDCI_33   |3             |          |NONE*    |NONE**     |         |       |LOCATED   |         |NO         |DRIVER          |
|W7        |                    |         |GND                   |         |           |              |          |         |           |         |       |          |         |           |                |
|W8        |                    |DIFFM    |IO_L92P_3             |UNUSED   |           |3             |          |         |           |         |       |          |         |           |                |
|W9        |                    |DIFFS    |IO_L48N_3             |UNUSED   |           |3             |          |         |           |         |       |          |         |           |                |
|W10       |                    |DIFFM    |IO_L51P_3             |UNUSED   |           |3             |          |         |           |         |       |          |         |           |                |
|W11       |                    |         |VCCO_3                |         |           |3             |          |         |           |         |3.30   |          |         |           |                |
|W12       |                    |         |VCCO_3                |         |           |3             |          |         |           |         |3.30   |          |         |           |                |
|W13       |                    |         |VCCINT                |         |           |              |          |         |           |         |1.5    |          |         |           |                |
|W14       |                    |         |VCCINT                |         |           |              |          |         |           |         |1.5    |          |         |           |                |
|W15       |                    |         |VCCINT                |         |           |              |          |         |           |         |1.5    |          |         |           |                |
|W16       |                    |         |VCCINT                |         |           |              |          |         |           |         |1.5    |          |         |           |                |
|W17       |                    |         |VCCINT                |         |           |              |          |         |           |         |1.5    |          |         |           |                |
|W18       |                    |         |VCCINT                |         |           |              |          |         |           |         |1.5    |          |         |           |                |
|W19       |                    |         |VCCINT                |         |           |              |          |         |           |         |1.5    |          |         |           |                |
|W20       |                    |         |VCCO_6                |         |           |6             |          |         |           |         |3.30   |          |         |           |                |
|W21       |                    |         |VCCO_6                |         |           |6             |          |         |           |         |3.30   |          |         |           |                |
|W22       |                    |DIFFM    |IO_L53P_6             |UNUSED   |           |6             |          |         |           |         |       |          |         |           |                |
|W23       |tv_in_ycrcb<9>      |IOB      |IO_L74P_6             |INPUT    |LVTTL      |6             |          |         |           |NONE     |       |LOCATED   |         |NO         |NONE            |
|W24       |                    |DIFFS    |IO_L71N_6             |UNUSED   |           |6             |          |         |           |         |       |          |         |           |                |
|W25       |                    |         |GND                   |         |           |              |          |         |           |         |       |          |         |           |                |
|W26       |ram0_ce_b           |IOB      |IO_L68P_6             |OUTPUT   |LVDCI_33   |6             |          |NONE*    |NONE**     |         |       |LOCATED   |         |NO         |DRIVER          |
|W27       |ram0_bwe_b<2>       |IOB      |IO_L54N_6             |OUTPUT   |LVDCI_33   |6             |          |NONE*    |NONE**     |         |       |LOCATED   |         |NO         |DRIVER          |
|W28       |ram0_data<12>       |IOB      |IO_L73N_6             |INPUT    |LVDCI_33   |6             |          |         |           |NONE     |       |LOCATED   |         |NO         |NONE            |
|W29       |ram0_data<13>       |IOB      |IO_L78P_6             |INPUT    |LVDCI_33   |6             |          |         |           |NONE     |       |LOCATED   |         |NO         |NONE            |
|W30       |ram0_address<8>     |IOB      |IO_L75N_6/VREF_6      |OUTPUT   |LVDCI_33   |6             |          |NONE*    |NONE**     |         |       |LOCATED   |         |NO         |DRIVER          |
|W31       |ram0_address<17>    |IOB      |IO_L76N_6             |OUTPUT   |LVDCI_33   |6             |          |NONE*    |NONE**     |         |       |LOCATED   |         |NO         |DRIVER          |
|Y1        |                    |DIFFM    |IO_L76P_3             |UNUSED   |           |3             |          |         |           |         |       |          |         |           |                |
|Y2        |ram1_data<9>        |IOB      |IO_L74P_3             |INPUT    |LVDCI_33   |3             |          |         |           |NONE     |       |LOCATED   |         |NO         |NONE            |
|Y3        |ram1_data<2>        |IOB      |IO_L71P_3             |INPUT    |LVDCI_33   |3             |          |         |           |NONE     |       |LOCATED   |         |NO         |NONE            |
|Y4        |ram1_data<1>        |IOB      |IO_L70P_3             |INPUT    |LVDCI_33   |3             |          |         |           |NONE     |       |LOCATED   |         |NO         |NONE            |
|Y5        |ram1_adv_ld         |IOB      |IO_L72N_3             |OUTPUT   |LVDCI_33   |3             |          |NONE*    |NONE**     |         |       |LOCATED   |         |NO         |DRIVER          |
|Y6        |ram1_address<13>    |IOB      |IO_L73P_3             |OUTPUT   |LVDCI_33   |3             |          |NONE*    |NONE**     |         |       |LOCATED   |         |NO         |DRIVER          |
|Y7        |ram1_address<2>     |IOB      |IO_L67N_3             |OUTPUT   |LVDCI_33   |3             |          |NONE*    |NONE**     |         |       |LOCATED   |         |NO         |DRIVER          |
|Y8        |ram1_address<1>     |IOB      |IO_L45N_3/VREF_3      |OUTPUT   |LVDCI_33   |3             |          |NONE*    |NONE**     |         |       |LOCATED   |         |NO         |DRIVER          |
|Y9        |ram1_clk            |IOB      |IO_L48P_3             |OUTPUT   |LVDCI_33   |3             |          |NONE*    |NONE**     |         |       |LOCATED   |         |NO         |DRIVER          |
|Y10       |                    |DIFFS    |IO_L27N_3/VREF_3      |UNUSED   |           |3             |          |         |           |         |       |          |         |           |                |
|Y11       |                    |         |VCCO_3                |         |           |3             |          |         |           |         |3.30   |          |         |           |                |
|Y12       |                    |         |VCCINT                |         |           |              |          |         |           |         |1.5    |          |         |           |                |
|Y13       |                    |         |VCCO_4                |         |           |4             |          |         |           |         |3.30   |          |         |           |                |
|Y14       |                    |         |VCCO_4                |         |           |4             |          |         |           |         |3.30   |          |         |           |                |
|Y15       |                    |         |VCCO_4                |         |           |4             |          |         |           |         |3.30   |          |         |           |                |
|Y16       |                    |         |VCCINT                |         |           |              |          |         |           |         |1.5    |          |         |           |                |
|Y17       |                    |         |VCCO_5                |         |           |5             |          |         |           |         |3.30   |          |         |           |                |
|Y18       |                    |         |VCCO_5                |         |           |5             |          |         |           |         |3.30   |          |         |           |                |
|Y19       |                    |         |VCCO_5                |         |           |5             |          |         |           |         |3.30   |          |         |           |                |
|Y20       |                    |         |VCCINT                |         |           |              |          |         |           |         |1.5    |          |         |           |                |
|Y21       |                    |         |VCCO_6                |         |           |6             |          |         |           |         |3.30   |          |         |           |                |
|Y22       |                    |DIFFS    |IO_L19N_6             |UNUSED   |           |6             |          |         |           |         |       |          |         |           |                |
|Y23       |                    |DIFFS    |IO_L44N_6             |UNUSED   |           |6             |          |         |           |         |       |          |         |           |                |
|Y24       |                    |DIFFM    |IO_L71P_6             |UNUSED   |           |6             |          |         |           |         |       |          |         |           |                |
|Y25       |ram0_address<6>     |IOB      |IO_L48N_6             |OUTPUT   |LVDCI_33   |6             |          |NONE*    |NONE**     |         |       |LOCATED   |         |NO         |DRIVER          |
|Y26       |ram0_address<7>     |IOB      |IO_L51N_6/VREF_6      |OUTPUT   |LVDCI_33   |6             |          |NONE*    |NONE**     |         |       |LOCATED   |         |NO         |DRIVER          |
|Y27       |ram0_data<17>       |IOB      |IO_L54P_6             |INPUT    |LVDCI_33   |6             |          |         |           |NONE     |       |LOCATED   |         |NO         |NONE            |
|Y28       |ram0_data<14>       |IOB      |IO_L73P_6             |INPUT    |LVDCI_33   |6             |          |         |           |NONE     |       |LOCATED   |         |NO         |NONE            |
|Y29       |ram0_data<15>       |IOB      |IO_L70N_6             |INPUT    |LVDCI_33   |6             |          |         |           |NONE     |       |LOCATED   |         |NO         |NONE            |
|Y30       |ram0_data<0>        |IOB      |IO_L75P_6             |INPUT    |LVDCI_33   |6             |          |         |           |NONE     |       |LOCATED   |         |NO         |NONE            |
|Y31       |ram0_address<9>     |IOB      |IO_L76P_6             |OUTPUT   |LVDCI_33   |6             |          |NONE*    |NONE**     |         |       |LOCATED   |         |NO         |DRIVER          |
+----------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------+

* Default value.
** This default Pullup/Pulldown value can be overridden in Bitgen. 
****** Special VCCO requirements may apply. Please consult the device 
       family datasheet for specific guideline on VCCO requirements. 


